Copy the Grading Quantities table from the Estimated Quantities sheet here.

Mainline

To edit the header, go to Insert -> Header -> Edit Header. The sheet numbers will be displayed automatically but fill in the rest of the required information.

In this space, paste the earthwork data from the log files created by GEOPAK. The data is best displayed in 9-point Consolas font, with margins set to “narrow”. These should be the default settings for this file. Paste data from the mainline, as well as each side road, driveway or special ditch. Separate each data set with copies of the text box above and use the text box to provide a description of each data set.