STANDARD TRAFFIC OPERATIONS DRAWINGS

DWG.	REV.	DESCRIPTION

DWG.	REV.	DESCRIPTION

DWG.	REV.	DESCRIPTION

SIGNS

T-S-6	02-12-91	STANDARD MOUNTING DETAILS - BOLTED EXTRUDED PANELS

T-S-7	02-12-91	HIGHWAY SHIELDS USED ON INTERSTATE AND U.S. NUMBERED ROUTES

T-S-8	07-15-91	HIGHWAY SHIELDS USED ON STATE NUMBERED ROUTES AND ARROWS

T-S-9	06-10-14	STANDARD LAYOUT GROUND MOUNTED SIGNS

T-S-10	04-04-12	STANDARD MOUNTING DETAILS FLAT SHEET SIGNS ALUMINUM-STEEL DESIGN

T-S-11	06-06-11	DELINEATOR AND MILEPOST DETAILS

T-S-12	07-10-17	STANDARD STEEL GROUND MOUNTED SIGNS, BREAK-AWAY TYPE POST FOOTING DETAILS, SQUARE TUBES

T-S-13	10-21-19	STANDARD STEEL GROUND MOUNTED SIGNS, BREAK-AWAY TYPE POST FOOTING DETAILS, I-BEAMS

T-S-14	10-21-19	STANDARD STEEL GROUND MOUNTED SIGNS, BREAK-AWAY TYPE POST FOOTING DETAILS, WF-BEAMS

T-S-15	12-07-90	STANDARD CONDUIT & GROUND DETAILS FOR OVERHEAD & CANTILEVER SIGN STRUCTURES

T-S-16	07-02-15	GROUND MOUNTED ROADSIDE SIGN PLACEMENT DETAILS

T-S-16A	07-02-15	GROUND MOUNTED ROADSIDE SIGN PLACEMENT DETAILS

T-S-17	07-11-17	STANDARD GROUND MOUNTED SIGN USING PERFORATED/KNOCKOUT SQUARE TUBE

T-S-18	02-14-14	END OF ROADWAY, DEAD END SIGNS, AND METAL BARRICADES (TYPE III)

T-S-19	06-12-20	STANDARD STEEL SIGN SUPPORTS

T-S-20	07-11-17	SIGN DETAILS

T-S-21	04-10-19	DETAILS FOR SIGNS MOUNTS ON CONCRETE MEDIAN BARRIERS

T-S-22	04-10-19	SIGN LAYOUT FOR HOV LANES

T-S-23A	07-11-17	MULTI-DIRECTIONAL SLIP BASE BREAKAWAY P-POST SIGN SUPPORT

T-S-23B	07-19-13	MULTI-DIRECTIONAL SLIP BASE BREAKAWAY STRUCTURAL PIPE SIGN SUPPORT

T-S-23C	07-02-15	BREAKAWAY POST SIGN SUPPORTS

T-S-24	08-02-13	DETAILS OF SIGN WITH SOLAR FLASHING ASSEMBLY

T-S-25	SIGNING PLAN DETAILS FOR ROUNDABOUTS

T-S-26	01-09-24	SIGNING PLAN FOR RESTRICTED CROSSING & J-TURN INTERSECTIONS

SIGNALS

T-SG-1	06-27-16	WOOD POLE DETAILS FOR SPAN MOUNTED SIGNALS

T-SG-2	06-27-16	LOOP LEAD-INS, CONDUIT AND PULL BOXES

T-SG-3	07-11-17	STANDARD NOTES AND DETAILS OF INDUCTIVE LOOPS

T-SG-3A	06-27-16	ALTERNATE DETECTION DETAILS

T-SG-4	06-27-16	SPAN WIRE AND MESSENGER CABLE DETAILS

T-SG-5	06-27-16	CONTROLLER CABINET DETAILS

T-SG-6	10-21-19	PEDESTRIAN SIGNAL DETAILS

T-SG-7	10-21-19	SIGNAL HEAD ASSEMBLIES

T-SG-7A	TYPICAL SIGNAL HEAD PLACEMENT APPROACHES

WITH NO THROUGH MOVEMENTS

T-SG-7B	10-21-19	TYPICAL SIGNAL HEAD PLACEMENT APPROACHES

WITH NO THROUGH MOVEMENTS

T-SG-7C	TYPICAL SIGNAL HEAD PLACEMENT

ONE-LANE AND TWO-LANE APPROACHES

T-SG-7D	10-21-19	TYPICAL SIGNAL HEAD PLACEMENT

TWO-LANE APPROACHES

T-SG-7E	TYPICAL SIGNAL HEAD PLACEMENT

THREE-LANE APPROACHES

T-SG-7F	07-13-17	TYPICAL SIGNAL HEAD PLACEMENT

THREE-LANE APPROACHES

T-SG-7G	TYPICAL SIGNAL HEAD PLACEMENT

THREE-LANE APPROACHES

T-SG-7H	10-21-19	TYPICAL SIGNAL HEAD PLACEMENT

THREE-LANE AND FOUR-LANE APPROACHES

T-SG-7HH	07-13-17	TYPICAL SIGNAL HEAD PLACEMENT

FOUR-LANE APPROACHES

T-SG-7J	TYPICAL SIGNAL HEAD PLACEMENT

FOUR-LANE APPROACHES

T-SG-7K	11-17-20	TYPICAL SIGNAL HEAD PLACEMENT

FOUR-LANE APPROACHES

T-SG-7L	10-21-19	TYPICAL SIGNAL HEAD PLACEMENT

FOUR-LANE APPROACHES

T-SG-7M	TYPICAL SIGNAL HEAD PLACEMENT

FIVE-LANE APPROACHES

T-SG-7N	TYPICAL SIGNAL HEAD PLACEMENT

FIVE-LANE APPROACHES

T-SG-7NN	07-13-17	TYPICAL SIGNAL HEAD PLACEMENT

FIVE-LANE APPROACHES

T-SG-7P	TYPICAL SIGNAL HEAD PLACEMENT

FIVE-LANE APPROACHES

T-SG-7PP	07-13-17	TYPICAL SIGNAL HEAD PLACEMENT

FIVE-LANE APPROACHES

T-SG-7R	TYPICAL SIGNAL HEAD PLACEMENT

SIX-LANE APPROACHES

T-SG-7S	10-21-19	TYPICAL SIGNAL HEAD PLACEMENT

SIX-LANE AND SEVEN-LANE APPROACHES

T-SG-8	06-27-16	STRAIN POLE DETAILS FOR SPAN MOUNTED SIGNALS

T-SG-9	10-21-19	DETAILS OF CANTILEVER SIGNAL SUPPORT

T-SG-9A	07-12-17	MISCELLANEOUS SIGNAL DETAILS

T-SG-10	07-11-17	MAST ARM POLE AND STRAIN POLES FOUNDATION DETAILS

T-SG-11	07-12-17	MAINTENANCE OF EXISTING SIGNALS DURING HIGHWAY CONSTRUCTION

T-SG-12	12-20-19	TYPICAL WIRING FOR SIGNAL HEADS AND DETECTION LOOPS

T-SG-13	06-27-16	FLASHING BEACON DETAIL

T-SG-14	PEDESTRIAN HYBRID BEACON DETAIL, 2 OR 3 LANE FACILITIES

T-SG-15	PEDESTRIAN HYBRID BEACON DETAIL, MULTILANE FACILITIES

LIGHTING AND UTILITY POLES

T-FO-1	FIBER OPTIC AERIAL ENTRANCE DETAILS

T-FO-2	FIBER OPTIC UNDERGROUND ENTRANCE DETAILS

T-FO-3	FIBER OPTIC AERIAL CONNECTION DETAILS

T-FO-4	FIBER OPTIC PULL BOX, CABINET & POLE DETAILS

T-L-1	11-17-20	STANDARD LIGHTING FOUNDATION DETAILS

T-L-1SA	09-11-13	STANDARD LIGHTING DETAILS FOR SINGLE ARM SUPPORTS

T-L-1TM	STANDARD LIGHTING DETAILS TENON MOUNTED OFFSET LIGHTING SUPPORTS

T-L-2	12-04-13	FOUNDATION DETAIL FOR LUMINAIRE MOUNTED ON CONCRETE MEDIAN BARRIER

T-L-3	04-15-96	STANDARD LIGHTING DETAILS PULL BOXES

T-L-4	05-25-11	STANDARD LIGHTING DETAILS CONDUIT, CABLE INSTALLATION

RAILROAD CROSSING

T-RR-1	11-01-11	TYPICAL PAVEMENT MARKING AT RAILROAD ACTIVE HIGHWAY GRADE CROSSINGS AND RAILROAD ADVANCE WARNING SIGN

T-RR-2	11-01-11	STANDARD DRAWING FOR RAILROAD AND HIGHWAY CROSSING SIGNAL WITH GATE

T-RR-3	11-01-11	STANDARD DRAWING FOR RAILROAD-HIGHWAY CROSSING SIGNAL

T-RR-4	11-01-11	STANDARD DRAWING FOR TYPICAL CURB & GUTTER PLAN FOR RAILROAD-HIGHWAY CROSSING WITH OR WITHOUT GATES

T-RR-5	11-01-11	RAILROAD-HIGHWAY CROSSING SIGNAL TYPICAL CANTILEVER SPAN

T-RR-6	10-25-13	TYPICAL SIGNING AND MARKING AT PASSIVE RAILROAD HIGHWAY GRADE CROSSINGS

STANDARD STRUCTURE DRAWINGS

NEW STRUCTURES

STD-1-1SS	05-10-21	BRIDGE RAILING SINGLE SLOPE CONCRETE PARAPET

STD-1-2	05-10-21	SLIDER PLATE AND DECK DRAIN

STD-1-2SS	05-10-21	SLIDER PLATES FOR SINGLE SLOPE PARAPETS AND DECK DRAINS

STD-1- 3	05-10-21	STD. CONCRETE MEDIAN BARRIER

STD-1-3SS	05-10-21	STD. SINGLE SLOPE CONCRETE MEDIAN BARRIER

STD-1-4	05-10-21	SLIDER PLATES FOR MEDIAN BARRIER

STD-1-4SS	05-10-21	SLIDER PLATE ASSEMBLIES FOR SINGLE SLOPE MEDIAN BARRIER

STD-1-5	06-05-23	PAVEMENT AT BRIDGE ENDS

STD-1-6	05-10-21	BRIDGE END DRAIN W/ PAVEMENT AT BRIDGE ENDS

STD-1-7	05-10-21	BRIDGE END DRAIN W/ PAVEMENT AT BRIDGE ENDS

STD-1-8	05-10-21	BRIDGE END DRAIN 2’ X 8’ 7” W/ PAVEMENT AT BRIDGE ENDS

STD-1-9	05-10-21	BRIDGE END DRAIN 4’ X 7” W/ PAVEMENT AT BRIDGE ENDS

STD-1-10	05-10-21	BRIDGE END DRAIN W/O PAVEMENT AT BRIDGE ENDS

STD-1-11	05-10-21	BRIDGE END DRAIN W/O PAVEMENT AT BRIDGE ENDS

STD-1-12	05-10-21	BRIDGE END DRAIN 2’x8’7” W/O PAVEMENT AT BRIDGE ENDS

STD-1-13	05-10-21	BRIDGE END DRAIN 4’x8’7” W/O PAVEMENT AT BRIDGE ENDS

STD-2-1	11-01-10	BRIDGE MOUNTED INTERCONNECTED PORTABLE BARRIER RAIL

STD-2-2	VERTICAL PANEL DETAILS

STD-2-3	BRIDGE MOUNTED INTERCONNECTED PORTABLE BARRIER RAIL ALTERNATE CONNECTION DETAIL

STD-3-1	11-01-10	STRIPSEAL EXPANSION JOINT

STD-3-2	11-01-10	STRIPSEAL EXPANSION JOINT

STD-4-1	04-08-05	STD. PRECAST PRESTRESSED BRIDGE DECK PANELS GENERAL DETAILS

STD-4-2	04-08-05	STD. PRECAST PRESTRESSED BRIDGE DECK PANELS DESIGN CRITERIA

STD-4-3	03-02-02	STD. PRECAST PRESTRESSED BRIDGE DECK PANELS GENERAL DETAILS

STD-4-4	06-10-96	STD. PRECAST PRESTRESSED BRIDGE DECK PANELS CONSTRUCTION DETAILS

STD-5-1	STD. PILE DETAILS

STD-5-2	STD. PILE DETAILS

STD-6-1	11-01-10	STANDARD SEISMIC DETAILS

STD-6-2	11-07-94	STANDARD SEISMIC DETAILS

STD-7-1	04-15-20	STD. CONCRETE RAIL

STD-8-2	11-01-10	LIGHT STANDARD SUPPORT DETAILS

STD-8-2SS	SINGLE SLOPE PARAPET STANDARD LIGHT SUPPORT DETAILS

STD-8-3	09-01-91	MEDIAN BARRIER LIGHT STANDARD SUPPORT DETAILS

STD-8-3SS	06-15-20	SINGLE SLOPE MEDIAN BARRIER STANDARD LIGHT SUPPORT DETAILS

STD-8-4	SIGN, LUMINAIRE, AND TRAFFIC SIGNAL SUPPORTS

STD-8-5	05-10-21	STANDARD PROTECTIVE FENCE DETAILS

STD-8-6	10-03-18	TRI-STAR STATE EMBLEM FINISH DETAILS

STD-9-1	10-07-08	REINFORCING BAR SUPPORT DETAILS FOR CONCRETE SLABS

STD-10-1	06-05-23	MISCELLANEOUS ABUTMENT AND DRAINAGE DETAILS

STD-10-2	06-05-23	MISC. ABUTMENT & PAVEMENT AT BRIDGE ENDS BACKFILL DETAILS

STD-10-3	01-10-24	STANDARD FLUME DETAILS

STD-11-1	04-15-20	BRIDGE RAILING W/ STRUCTURAL TUBING

STD-11-2	04-15-20	STANDARD CONCRETE CLASSIC RAIL 2007

STD-11-3	04-15-20	STANDARD CONCRETE PEDESTRIAN CLASSIC RAIL

STD-11-4	CONCRETE CLASSIC RAIL (42” TALL)

STD-11-4A	CONCRETE CLASSIC RAIL (42” TALL)

STD-14-1	06-05-23	STD. DETAILS AND INT. DIAPH. DETAILS FOR BULB - TEE BEAMS

STD-14-1A	STANDARD DETAILS AND INTERMEDIATE DIAPHRAGM DETAILS FOR BULB-TEE BEAMS (8" WEBS)

STD-14-2	STD. DETAILS AND INT. DIAPH. DETAILS FOR I-BEAMS

STD-14-3	STD. DETAILS FOR PRESTRESSED BOX BEAMS

LRFD BOX CULVERTS

(See Section 4-604.00)

This section is for all projects having either concrete box and/or slab culverts or bridges projects that began preliminary engineering After October 2010.

STD-17-1	INDEX OF DRAWINGS

STD-17-2	TERMINOLOGY

STD-17-3	GENERAL NOTES

STD-17-4	DESIGN SECTION LIMITS

STD-17-5	TYPICAL SECTION AND DETAILS

STD-17-6	TYPICAL ELEVATIONS

STD-17-7	CURB, RAIL & EDGE BEAM DETAILS - SKEW NOT LESS THAN 45 DEG.

STD-17-8	EDGE BEAM DETAILS FOR FILLS GREATER THAN 3’ - 6”

STD-17-9	INTERIOR WALL END TREATMENTS

STD-17-10	TYPICAL WINGWALL DETAILS AND NOTES

STD-17-11	WINGWALL DIMENSIONS AND QUANTITIES

STD-17-12	WINGWALL DIMENSIONS AND QUANTITIES

STD-17-13	WINGWALL DIMENSIONS AND QUANTITIES

STD-17-14	WINGWALL DIMENSIONS AND QUANTITIES

STD-17-15	WINGWALL & SPECIAL RETAINING WALL DESIGN SECTIONS

STD-17-16	WINGWALL DESIGN SECTION

STD-17-17	06-01-11	BACKFILL AND DRAINAGE DETAILS

STD-17-18	BACKFILL DETAILS

STD-17-19	06-20-18	PAVED OUTLET DETAIL

STD-17-20	LOW FLOW CHANNEL CONSTRUCTION DETAILS FOR CULVERT INLET AND OUTLET

STD-17-21	DEBRIS DEFLECTION WALL FOR BOX BRIDGE

STD-17-22	DEBRIS DEFLECTION WALL FOR SLAB BRIDGE

STD-17-23	SIDEWALK AND MISCELLANEOUS DETAILS

STD-17-24	WARPED SLOPE DETAIL

STD-17-25	STAGE CONSTRUCTION JOINT DETAIL (FILL ABOVE TOP OF SLAB NOT GREATER THAN 3’-6”)

STD-17-26	EXTENSION DETAILS

STD-17-27	EXTENSION DETAILS FOR SCOURED OUTLET

STD-17-28	END SECTION DETAILS

STD-17-29	PRECAST BOX CULVERT DETAILS

STD-17-34	INTERNAL ENERGY DISSIPATOR FOR BOX AND PIPE CULVERTS

STD-17-51	05-01-14	BOX BRIDGE, 1 BARREL AT 6’, CLEAR HTS. 3’ - 6’, 0 - 60’ FILL

STD-17-52	BOX BRIDGE, 1 BARREL AT 8’, CLEAR HTS. 3’ - 5’, 0 - 60’ FILL

STD-17-53	BOX BRIDGE, 1 BARREL AT 8’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-54	BOX BRIDGE, 1 BARREL AT 10’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-55	BOX BRIDGE, 1 BARREL AT 10’, CLEAR HTS. 7’ - 10’, 0 - 60’ FILL

STD-17-56	BOX BRIDGE, 1 BARREL AT 12’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-57	BOX BRIDGE, 1 BARREL AT 12’, CLEAR HTS. 7’ - 9’, 0 - 60’ FILL

STD-17-58	BOX BRIDGE, 1 BARREL AT 12’, CLEAR HTS. 10’ - 12’, 0 - 60’ FILL

STD-17-59	BOX BRIDGE, 1 BARREL AT 14’, CLEAR HTS. 5’ - 7’, 0 - 60’ FILL

STD-17-60	BOX BRIDGE, 1 BARREL AT 14’, CLEAR HTS. 8’ - 11’, 0 - 60’ FILL

STD-17-61	BOX BRIDGE, 1 BARREL AT 14’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-62	BOX BRIDGE, 1 BARREL AT 16’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-63	BOX BRIDGE, 1 BARREL AT 16’, CLEAR HTS. 9’ - 12’, 0 - 60’ FILL

STD-17-64	BOX BRIDGE, 1 BARREL AT 16’, CLEAR HTS. 13’ - 16’, 0 - 60’ FILL

STD-17-65	BOX BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-66	BOX BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 9’ - 11’, 0 - 60’ FILL

STD-17-67	BOX BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-68	BOX BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 15’ - 18’, 0 - 60’ FILL

STD-17-71	05-01-14	BOX BRIDGE, 2 BARRELS AT 6’, CLEAR HTS. 3’ - 6’, 0 - 60’ FILL

STD-17-72	BOX BRIDGE, 2 BARRELS AT 8’, CLEAR HTS. 3’ - 5’, 0 - 60’ FILL

STD-17-73	BOX BRIDGE, 2 BARRELS AT 8’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-74	BOX BRIDGE, 2 BARRELS AT 10’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-75	BOX BRIDGE, 2 BARRELS AT 10’, CLEAR HTS. 7’ - 10’, 0 - 60’ FILL

STD-17-76	BOX BRIDGE, 2 BARRELS AT 12’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-77	BOX BRIDGE, 2 BARRELS AT 12’, CLEAR HTS. 7’ - 9’, 0 - 60’ FILL

STD-17-78	BOX BRIDGE, 2 BARRELS AT 12’, CLEAR HTS. 10’ - 12’, 0 - 60’ FILL

STD-17-79	BOX BRIDGE, 2 BARRELS AT 14’, CLEAR HTS. 5’ - 7’, 0 - 60’ FILL

STD-17-80	BOX BRIDGE, 2 BARRELS AT 14’, CLEAR HTS. 8’ - 11’, 0 - 60’ FILL

STD-17-81	BOX BRIDGE, 2 BARRELS AT 14’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-82	BOX BRIDGE, 2 BARRELS AT 16’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-83	BOX BRIDGE, 2 BARRELS AT 16’, CLEAR HTS. 9’ - 12’, 0 - 60’ FILL

STD-17-84	BOX BRIDGE, 2 BARRELS AT 16’, CLEAR HTS. 13’ - 16’, 0 - 60’ FILL

STD-17-85	BOX BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-86	BOX BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 9’ - 11’, 0 - 60’ FILL

STD-17-87	BOX BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-88	BOX BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 15’ - 18’, 0 - 60’ FILL

STD-17-91	BOX BRIDGE, 3 BARRELS AT 6’, CLEAR HTS. 3’ - 6’, 0 - 60’ FILL

STD-17-92	BOX BRIDGE, 3 BARRELS AT 8’, CLEAR HTS. 3’ - 5’, 0 - 60’ FILL

STD-17-93	BOX BRIDGE, 3 BARRELS AT 8’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-94	BOX BRIDGE, 3 BARRELS AT 10’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-95	BOX BRIDGE, 3 BARRELS AT 10’, CLEAR HTS. 7’ - 10’, 0 - 60’ FILL

STD-17-96	BOX BRIDGE, 3 BARRELS AT 12’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-97	BOX BRIDGE, 3 BARRELS AT 12’, CLEAR HTS. 7’ - 9’, 0 - 60’ FILL

STD-17-98	BOX BRIDGE, 3 BARRELS AT 12’, CLEAR HTS. 10’ - 12’, 0 - 60’ FILL

STD-17-99	BOX BRIDGE, 3 BARRELS AT 14’, CLEAR HTS. 5’ - 7’, 0 - 60’ FILL

STD-17-100	BOX BRIDGE, 3 BARRELS AT 14’, CLEAR HTS. 8’ - 11’, 0 - 60’ FILL

STD-17-101	BOX BRIDGE, 3 BARRELS AT 14’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-102	BOX BRIDGE, 3 BARRELS AT 16’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-103	BOX BRIDGE, 3 BARRELS AT 16’, CLEAR HTS. 9’ - 12’, 0 - 60’ FILL

STD-17-104	BOX BRIDGE, 3 BARRELS AT 16’, CLEAR HTS. 13’ - 16’, 0 - 60’ FILL

STD-17-105	BOX BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-106	BOX BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 9’ - 11’, 0 - 60’ FILL

STD-17-107	BOX BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-108	BOX BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 15’ - 18’, 0 - 60’ FILL

STD-17-111	SLAB BRIDGE, 1 BARREL AT 6’, CLEAR HTS. 3’ - 6’, 0 - 60’ FILL

STD-17-112	SLAB BRIDGE, 1 BARREL AT 8’, CLEAR HTS. 3’ - 5’, 0 - 60’ FILL

STD-17-113	SLAB BRIDGE, 1 BARREL AT 8’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-114	SLAB BRIDGE, 1 BARREL AT 10’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-115	SLAB BRIDGE, 1 BARREL AT 10’, CLEAR HTS. 7’ - 10’, 0 - 60’ FILL

STD-17-116	SLAB BRIDGE, 1 BARREL AT 12’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-117	SLAB BRIDGE, 1 BARREL AT 12’, CLEAR HTS. 7’ - 9’, 0 - 60’ FILL

STD-17-118	SLAB BRIDGE, 1 BARREL AT 12’, CLEAR HTS. 10’ - 12’, 0 - 60’ FILL

STD-17-119	SLAB BRIDGE, 1 BARREL AT 14’, CLEAR HTS. 5’ - 7’, 0 - 60’ FILL

STD-17-120	SLAB BRIDGE, 1 BARREL AT 14’, CLEAR HTS. 8’ - 11’, 0 - 60’ FILL

STD-17-121	SLAB BRIDGE, 1 BARREL AT 14’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-122	SLAB BRIDGE, 1 BARREL AT 16’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-123	SLAB BRIDGE, 1 BARREL AT 16’, CLEAR HTS. 9’ - 12’, 0 - 60’ FILL

STD-17-124	SLAB BRIDGE, 1 BARREL AT 16’, CLEAR HTS. 13’ - 16’, 0 - 60’ FILL

STD-17-125	SLAB BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-126	SLAB BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 9’ - 11’, 0 - 60’ FILL

STD-17-127	SLAB BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-128	SLAB BRIDGE, 1 BARREL AT 18’, CLEAR HTS. 15’ - 18’, 0 - 60’ FILL

STD-17-131	SLAB BRIDGE, 2 BARRELS AT 6’, CLEAR HTS. 3’ - 6’, 0 - 60’ FILL

STD-17-132	SLAB BRIDGE, 2 BARRELS AT 8’, CLEAR HTS. 3’ - 5’, 0 - 60’ FILL

STD-17-133	SLAB BRIDGE, 2 BARRELS AT 8’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-134	SLAB BRIDGE, 2 BARRELS AT 10’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-135	SLAB BRIDGE, 2 BARRELS AT 10’, CLEAR HTS. 7’ - 10’, 0 - 60’ FILL

STD-17-136	SLAB BRIDGE, 2 BARRELS AT 12’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-137	SLAB BRIDGE, 2 BARRELS AT 12’, CLEAR HTS. 7’ - 9’, 0 - 60’ FILL

STD-17-138	SLAB BRIDGE, 2 BARRELS AT 12’, CLEAR HTS. 10’ - 12’, 0 - 60’ FILL

STD-17-139	SLAB BRIDGE, 2 BARRELS AT 14’, CLEAR HTS. 5’ - 7’, 0 - 60’ FILL

STD-17-140	SLAB BRIDGE, 2 BARRELS AT 14’, CLEAR HTS. 8’ - 11’, 0 - 60’ FILL

STD-17-141	SLAB BRIDGE, 2 BARRELS AT 14’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-142	SLAB BRIDGE, 2 BARRELS AT 16’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-143	SLAB BRIDGE, 2 BARRELS AT 16’, CLEAR HTS. 9’ - 12’, 0 - 60’ FILL

STD-17-144	SLAB BRIDGE, 2 BARRELS AT 16’, CLEAR HTS. 13’ - 16’, 0 - 60’ FILL

STD-17-145	SLAB BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-146	SLAB BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 9’ - 11’, 0 - 60’ FILL

STD-17-147	SLAB BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-148	SLAB BRIDGE, 2 BARRELS AT 18’, CLEAR HTS. 15’ - 18’, 0 - 60’ FILL

STD-17-151	SLAB BRIDGE, 3 BARRELS AT 6’, CLEAR HTS. 3’ - 6’, 0 - 60’ FILL

STD-17-152	SLAB BRIDGE, 3 BARRELS AT 8’, CLEAR HTS. 3’ - 5’, 0 - 60’ FILL

STD-17-153	SLAB BRIDGE, 3 BARRELS AT 8’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-154	SLAB BRIDGE, 3 BARRELS AT 10’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-155	SLAB BRIDGE, 3 BARRELS AT 10’, CLEAR HTS. 7’ - 10’, 0 - 60’ FILL

STD-17-156	SLAB BRIDGE, 3 BARRELS AT 12’, CLEAR HTS. 4’ - 6’, 0 - 60’ FILL

STD-17-157	SLAB BRIDGE, 3 BARRELS AT 12’, CLEAR HTS. 7’ - 9’, 0 - 60’ FILL

STD-17-158	SLAB BRIDGE, 3 BARRELS AT 12’, CLEAR HTS. 10’ - 12’, 0 - 60’ FILL

STD-17-159	SLAB BRIDGE, 3 BARRELS AT 14’, CLEAR HTS. 5’ - 7’, 0 - 60’ FILL

STD-17-160	SLAB BRIDGE, 3 BARRELS AT 14’, CLEAR HTS. 8’ - 11’, 0 - 60’ FILL

STD-17-161	SLAB BRIDGE, 3 BARRELS AT 14’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-162	SLAB BRIDGE, 3 BARRELS AT 16’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-163	SLAB BRIDGE, 3 BARRELS AT 16’, CLEAR HTS. 9’ - 12’, 0 - 60’ FILL

STD-17-164	SLAB BRIDGE, 3 BARRELS AT 16’, CLEAR HTS. 13’ - 16’, 0 - 60’ FILL

STD-17-165	SLAB BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 6’ - 8’, 0 - 60’ FILL

STD-17-166	SLAB BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 9’ - 11’, 0 - 60’ FILL

STD-17-167	SLAB BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 12’ - 14’, 0 - 60’ FILL

STD-17-168	SLAB BRIDGE, 3 BARRELS AT 18’, CLEAR HTS. 15’ - 18’, 0 - 60’ FILL

BRIDGE REPAIRS

SBR-2-115	06-15-16	GENERAL NOTES AND DETAILS FOR EXPANSION JOINT REPLACEMENT CONSTRUCTION TYPES “A” THRU “J” - 1991

SBR-2-116	01-04-96	GENERAL DETAILS FOR STRIPSEAL EXPANSION JOINT REPLACEMENT CONSTRUCTION DETAILS TYPES “A” THRU “J” - 1991

SBR-2-117	05-30-96	STRIPSEAL EXPANSION JOINTS - REPLACEMENT CONSTRUCTION DETAILS TYPE “A” AND TYPE “B” - 1991

SBR-2-118	05-30-96	STRIPSEAL EXPANSION JOINT REPLACEMENT CONSTRUCTION DETAILS TYPE “C” AND TYPE “D” - 1991

SBR-2-119	05-30-96	STRIPSEAL EXPANSION JOINT REPLACEMENT CONSTRUCTION DETAILS TYPE “E” AND TYPE “F” - 1991

SBR-2-120	05-30-96	STRIPSEAL EXPANSION JOINT REPLACEMENT CONSTRUCTION DETAILS TYPE “G” AND “H” - 1991

SBR-2-121	01-04-96	STRIPSEAL EXPANSION JOINT REPLACEMENT CONSTRUCTION DETAILS TYPE “J” - 1991

SBR-2-122	01-04-96	DETAILS FOR PRECAST SLAB BRIDGE CHANNELS, SPANS 16’ - 0” THRU 34’ - 0”, DEGREE OF SKEW 90 - 75 - 60 - 45 - 1992

SBR-2-123	01-04-96	DETAILS FOR PRECAST SLAB BRIDGE CHANNELS, SPANS 16’ - 0” THRU 34’ -0”, DEGREE OF SKEW 90 - 75 - 60 - 45 - 1992

SBR-2-124	01-04-96	DETAILS SHOWING REPLACEMENT OF EXISTING BRIDGERAIL SYSTEM WITH NEW JERSEY SHAPE CONCRETE PARAPET AND NEW 10’ -2” ENDPOST - 1988

SBR-2-125	11-05-01	DETAILS SHOWING REPLACEMENT OF EXISTING BRIDGERAIL SYSTEM WITH NEW JERSEY SHAPE CONCRETE PARAPET AND NEW 10’ -2” ENDPOST - 1988

SBR-2-126	01-04-96	DETAILS SHOWING REPLACEMENT OF EXISTING BRIDGERAIL SYSTEM WITH NEW JERSEY SHAPE CONCRETE PARAPET AND NEW 10’ -2” ENDPOST - 1988

SBR-2-127	11-05-01	DETAILS SHOWING PIER PROTECTION WITH NEW CONCRETE BARRIER WALL - 1988

SBR-2-128	01-04-96	DETAILS SHOWING PIER PROTECTION WITH NEW CONCRETE BARRIER WALL - 1988

SBR-2-129	11-05-01	DETAILS SHOWING PIER PROTECTION WITH NEW VERTICAL CONCRETE BARRIER - 1988

SBR-2-130	01-04-96	DETAILS SHOWING PIER PROTECTION WITH NEW VERTICAL CONCRETE BARRIER - 1988

SBR-2-131	01-22-02	DETAILS SHOWING GUARDRAIL ATTACHMENT AT BRIDGE ENDS TO EXISTING CONCRETE SLOPE FACE ENDPOST - 1989

SBR-2-132	01-04-96	DETAILS SHOWING GUARDRAIL ATTACHMENT AT BRIDGE ENDS EXISTING CONCRETE SLOPE FACE ENDPOST - 1989

SBR-2-133	01-22-02	DETAILS SHOWING GUARDRAIL ATTACHMENT AT BRIDGE ENDS TO EXISTING CONCRETE VERTICAL FACE ENDPOST - 1989

SBR-2-134	01-04-96	DETAILS SHOWING GUARDRAIL ATTACHMENT AT BRIDGE ENDS TO EXISTING CONCRETE VERTICAL FACE ENDPOST - 1989

SBR-2-135	01-22-02	GUARDRAIL ATTACHMENT TO EXISTING PIER PROTECTION - 1991

SBR-2-136	11-05-01	STANDARD DRAWING FOR REPLACING EXISTING CONCRETE ENDPOST AND GUARDRAIL AT EXISTING BRIDGE ENDS - 1992

SBR-2-137	11-05-01	STANDARD SHOWING DETAILS FOR ATTACHING NEW GUARDRAIL TO EXISTING END OF BRIDGE - 1992

SBR-2-138	11-05-01	STANDARD SHOWING DETAILS FOR ATTACHING NEW GUARDRAIL AT EXISTING BRIDGE END AND ALONG EXISTING BRIDGE RAIL - 1992

SBR-2-140	11-05-01	STANDARD SHOWING DETAILS FOR ATTACHING NEW GUARDRAIL ALONG EXISTING BRIDGE RAILS - 1992

SBR-2-144	01-22-02	STANDARD SHOWING DETAILS OF ATTACHING GUARDRAIL BRIDGERAIL TO TOP OF EXISTING CURBS – 1992