STANDARD ROADWAY DRAWINGS

DWG. NO.	REV.	DESCRIPTION

DWG. NO.	REV.	DESCRIPTION

DWG. NO.	REV.	DESCRIPTION

10-100.00 STANDARD ROADWAY TITLE SHEET, ABBREVIATIONS, AND LEGENDS

10-100.01	STANDARD ROADWAY DRAWINGS TITLE SHEET

RD-TP-1	10-01-24	STANDARD ROADWAY DRAWINGS TITLE SHEET

10-100.02	STANDARD ABBREVIATIONS AND LEGENDS

RD-A-1	02-20-20	STANDARD ABBREVIATIONS A THROUGH L

RD-A-2	STANDARD ABBREVIATIONS M THROUGH Z

RD-L-1	02-20-20	STANDARD LEGEND

RD-L-1A	STANDARD LEGEND

RD-L-2	02-20-20	STANDARD LEGEND FOR UTILITY INSTALLATIONS

RD-L-3	03-01-23	STANDARD LEGEND FOR SIGNALIZATION AND LIGHTING

RD-L-4	10-01-24	STANDARD LEGEND FOR SIGNALIZATION AND LIGHTING

RD-L-5	07-30-24	STANDARD LEGEND FOR EROSION PREVENTION AND SEDIMENT CONTROL

RD-L-6	02-20-20	STANDARD LEGEND FOR EROSION PREVENTION AND SEDIMENT CONTROL

RD-L-7	02-20-20	STANDARD LEGEND FOR EROSION PREVENTION AND SEDIMENT CONTROL

RD-L-8	02-20-20	STANDARD LEGEND FOR NATURAL STREAM DESIGN

10-101.00 STANDARDS ROADWAY DRAWINGS

10-101.01	RD18 ROUNDABOUT TYPICAL SECTIONS AND DESIGN CRITERIA

RD18-RTS-1	DESIGN STANDARDS FOR SINGLE LANE URBAN AND RURAL ROUNDABOUTS

RD18-RTS-2	DESIGN STANDARDS FOR MULTI-LANE URBAN AND RURAL ROUNDABOUTS

RD18-RTS-3	04-30-25	STANDARD CONSTRUCTION DETAILS FOR ROUNDABOUTS

RD18-RSD-1	SIGHT DISTANCE FOR URBAN AND RURAL ROUNDABOUT

10-101.02	RD11 TYPICAL SECTIONS AND DESIGN CRITERIA

RD11-SE-1	TRANSITION AND CROSS SLOPE DETAILS

RD11-SE-2	SUPERELEVATION TRANSITION DETAILS FOR UNDIVIDED ROADWAYS

RD11-SE-2A	SUPERELEVATION TRANSITION SECTIONS FOR UNDIVIDED ROADWAYS

RD11-SE-3	SUPERELEVATION TRANSITION DETAILS FOR DIVIDED ROADWAYS

RD11-SE-3A	SUPERELEVATION TRANSITION SECTIONS FOR DIVIDED ROADWAYS

RD11-TS-1	06-28-19	DESIGN STANDARDS FOR LOW-VOLUME ROADS

RD11-TS-1A	06-28-19	DESIGN STANDARDS FOR LOCAL ROADS AND STREETS

RD11-TS-2	DESIGN STANDARDS FOR COLLECTORS, 2-LANE ROADS AND STREETS

RD11-TS-2A	DESIGN STANDARDS FOR COLLECTOR HIGHWAYS WITH DEPRESSED MEDIAN (4 AND 6 LANE)

RD11-TS-2B	DESIGN STANDARDS FOR COLLECTOR HIGHWAYS WITH FLUSH MEDIAN (4 AND 6 LANE)

RD11-TS-3	DESIGN STANDARD FOR ARTERIAL HIGHWAYS (2-LANE)

RD11-TS-3A	06-28-19	DESIGN STANDARDS FOR ARTERIAL HIGHWAYS WITH DEPRESSED MEDIAN (4 AND 6 LANE)

RD11-TS-3B	DESIGN STANDARDS FOR ARTERIAL HIGHWAYS WITH FLUSH MEDIAN (4 AND 6 LANE)

RD11-TS-3C	DESIGN STANDARDS FOR ARTERIALS WITH INDEPENDENT ROADWAYS (4 AND 6 LANE)

RD11-TS-4	10-01-24	DESIGN STANDARDS FOR ARTERIAL AND FREEWAY RAMPS (1, 2 AND 3 LANE)

RD11-TS-5	06-28-19	DESIGN STANDARDS FOR FREEWAYS WITH DEPRESSED MEDIAN (4 AND 6 LANE)

RD11-TS-5A	DESIGN STANDARDS FOR FREEWAYS WITH INDEPENDENT ROADWAYS (4 AND 6 LANE)

RD11-TS-5B	DESIGN STANDARDS FOR FREEWAYS WITH MEDIAN BARRIER (4 AND 6 LANE)

RD11-TS-5W	06-15-21	TYPICAL DETAIL FOR INSIDE LANE WIDENING OF FREEWAYS

RD11-TS-6	TYPICAL CURB & GUTTER SECTIONS WITH SHOULDERS AND WITH GRASS STRIPS

RD11-TS-6A	TYPICAL CURB & GUTTER SECTIONS WITHOUT SHOULDERS AND WITH GRASS STRIPS

RD11-TS-6B	TYPICAL CURB AND GUTTER SECTIONS WITH SHOULDERS AND WITHOUT GRASS STRIPS

RD11-TS-6C	TYPICAL CURB AND GUTTER SECTIONS WITHOUT SHOULDERS AND WITHOUT GRASS STRIPS

RD11-TS-7	07-17-20	DESIGN STANDARDS 2-LANE CURB & GUTTER WITH CONTINUOUS 2-WAY LEFT-TURN LANE WITHOUT GRASS STRIPS

RD11-TS-7A	07-17-20	DESIGN STANDARDS 2-LANE CURB & GUTTER WITH CONTINUOUS 2-WAY LEFT-TURN LANE WITH GRASS STRIPS

RD11-TS-7B	07-17-20	DESIGN STANDARDS 2-LANE HIGHWAYS WITH CONTINUOUS 2-WAY LEFT-TURN LANE

10-101.03	RD11 SLOPE DEVELOPMENT AND RUNOFF LENGTHS

RD11-LR-1	MINIMUM RUNOFF LENGTHS (LR) FOR URBAN HIGHWAYS

RD11-LR-2	MINIMUM RUNOFF LENGTHS (LR) FOR RURAL HIGHWAYS

RD11-S-11	DESIGN AND CONSTRUCTION DETAILS FOR ROADSIDE SLOPE DEVELOPMENT

RD11-S-11A	ROADSIDE DITCH DETAILS FOR DESIGN AND CONSTRUCTION

RD11-S-11B	DESIGN AND CONSTRUCTION DETAILS FOR ROCK CUT SLOPE AND CATCHMENT

RD11-SA-1	01-09-24	SAFETY APPROACH TO UNDERPASSES GRADING DESIGN AND SLOPE PROTECTION

10-101.04	RD11 INTERSECTION SIGHT DISTANCE

RD11-SD-1	INTERSECTION SIGHT DISTANCE DESIGN AND GENERAL NOTES

RD11-SD-2	INTERSECTION SIGHT DISTANCE LANDSCAPE AND OBSTRUCTION

RD11-SD-3	INTERSECTION SIGHT DISTANCE 2-LANE ROADWAYS

RD11-SD-4	INTERSECTION SIGHT DISTANCE 4-LANE AND 5-LANE UNDIVIDED ROADWAYS

RD11-SD-5	INTERSECTION SIGHT DISTANCE 4-LANE DIVIDED HIGHWAYS

RD11-SD-6	INTERSECTION SIGHT DISTANCE 6-LANE DIVIDED HIGHWAYS

RD11-SD-7	INTERSECTION SIGHT DISTANCE FOR PASSIVE RAILROAD HIGHWAY GRADE CROSSINGS

10-101.05	UNDERDRAINS

RD-UD-3	01-09-24	UNDERDRAIN DETAILS

RD-UD-4	06-28-19	UNDERDRAIN LATERAL DETAILS

RD-UD-6	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 1:1 & 2:1 SLOPES

RD-UD-7	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 3:1 & 4:1 SLOPES

RD-UD-8	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 5:1 SLOPES

RD-UD-9	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 6:1 SLOPES

10-102.00 PIPE CULVERTS, ENDWALLS, AND ENERGY DISSIPATERS

10-102.01	PIPE CULVERTS AND FLUME

D-FLU-1	06-28-19	FLUME DETAILS

D-FLU-2	BRIDGE END DRAIN FLUME DETAILS

D-FLU-2A	BRIDGE END DRAIN FLUME DETAILS

D-FLU-3	04-01-25	BRIDGE END DRAIN FLUME DETAILS

D-PB-1	03-01-23	STANDARD DETAILS FOR CONCRETE PIPE INSTALLATION

D-PB-2	03-01-23	STANDARD DETAILS FOR FLEXIBLE PIPE INSTALLATION

D-PB-3	11-30-20	INDUCED TRENCH SOIL EMBANKMENT FOR PIPE CULVERT INSTALLATION

D-PB-4	01-09-24	PIPE COLLAR DETAILS

D-PG-3	06-28-19	FERROUS AND ALUMINUM CORRUGATED METAL PIPE

D-PG-4	06-28-19	FERROUS AND ALUMINUM CORRUGATED METAL PIPE ARCHES

D-PO-1	06-28-19	STANDARD OVAL AND REINFORCED CONCRETE ARCH PIPE CULVERT

D-PS-1	06-28-19	STRUTTING DETAILS FOR CORR. METAL & STRUCTURAL PLATE ROUND PIPE

10-102.02	SAFETY CROSS DRAIN ENDWALLS

D-PE-15A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 15" PIPE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-15B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 15" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-18A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 18" PIPE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-18B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 18" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-24A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 24" PIPE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-24B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 24" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-30A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 30" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-30B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 30" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-36A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 36" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-36B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 36" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-42A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 42" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-42B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 42" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-48A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 48" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-48B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 48" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-99	03-04-21	TYPE "U" CROSS DRAIN ENDWALL DETAILS, PIPE GRATE & SKEWED CONNECTION

10-102.03	SAFETY SIDE DRAIN ENDWALLS

D-SEW-1A	07-07-23	TYPE "SAFETY" SIDE ENDWALL WITH STEEL PIPE GRATE, FOR 15" THRU 48" PIPES, 6:1 SLOPE

D-SEW-12D	07-07-23	TYPE “SAFETY” SIDE DRAIN ENDWALL WITH STEEL PIPE GRATE, FOR 18” PIPE, 12:1 SLOPE

SD-MSE-1	06-28-19	SIDE DRAIN MITERED END SECTION

10-102.04	PROTECTED ENDWALLS*

NOTE: THE PROTECTED ENDWALLS MAY NOT BE USED INSIDE THE CLEAR ZONE UNLESS SHIELDED BY GUARDRAIL OR OTHER SAFETY DEVICE.

D-PE-4	06-28-19	STRAIGHT CONCRETE ENDWALLS (PIPE SIZES 18" TO 30")

D-PE-5	06-28-19	STRAIGHT CONCRETE ENDWALLS FOR HORIZONTAL OVAL CONCRETE PIPES (ALL SIZES AND SKEWS)

D-PEW-1	PROTECTED ENDWALLS FOR ROUND & OVAL PIPES (PIPE SIZES 18” TO 72”, ALL SKEWS, 2:1 & 3:1 SLOPES)

D-PEW-2	PROTECTED ENDWALLS FOR ROUND PIPES DETAILS & QUANTITIES (PIPE SIZES 18” TO 72”, ALL SKEWS, 2:1 & 3:1 SLOPES)

D-PEW-3	PROTECTED ENDWALLS FOR OVAL PIPES DETAILS & QUANTITIES (EQU. PIPE SIZES 18” TO 72”, ALL SKEWS, 2:1 & 3:1 SLOPES)

D-PEW-4	PROTECTED STRAIGHT ENDWALLS (PIPE SIZES 18” TO 30” & EQU. OVAL PIPES)

D-PEW-5	RIP-RAP END TREATMENT FOR CORRUGATED METAL PIPE, OVAL AND PIPE ARCH CULVERTS WITH BEVELED ENDS (PIPE SIZES 42” & LARGER)

10-102.05	ENERGY DISSIPATERS

D-ED-1	CONCRETE FLUME ENERGY DISSIPATER

10-103.00 CATCH BASINS AND MANHOLES

10-103.01	CATCH BASINS

D-CB-DI	ALTERNATE CATCH BASIN DROP INLET DETAILS

D-CB-10LPC	02-20-20	LOW PROFILE LOWERED CURB 32" X 26" RECTANGULAR CONCRETE NO. 10LPC CATCH BASIN

D-CB-10RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 10 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-10S	02-20-20	STANDARD RECTANGULAR CONCRETE N0. 10 CATCH BASIN

D-CB-10SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 10 CATCH BASIN

D-CB-12LP	02-20-20	LOW PROFILE 32" X 32" SQUARE CONCRETE NO. 12LP CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12LPA	ALTERNATE REINFORCEMENT FOR PRECAST CONCRETE 32” X 32” NO. 12LP CATCH BASIN

D-CB-12P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO.12 CATCH BASIN

D-CB-12RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 12 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12RB	02-20-20	STANDARD PRECAST 60" AND 72" CIRCULAR NO. 12 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12RC	02-20-20	STANDARD PRECAST 84" THRU 120" CIRCULAR NO. 12 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 12 CATCH BASIN

D-CB-12SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-12SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-12SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-12SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-13P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 13 CATCH BASIN

D-CB-13RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 13 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-13RB	02-20-20	STANDARD PRECAST 60" AND 72" CIRCULAR NO. 13 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-13RC	02-20-20	STANDARD PRECAST 84" THRU 120" CIRCULAR NO. 13 CATCH BASIN (FOR USE WITH 6" VERTICAL CURB)

D-CB-13S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 13 CATCH BASIN

D-CB-14P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 14 CATCH BASIN

D-CB-14RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 14RB CATCH BASIN

D-CB-14S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 14 CATCH BASIN

D-CB-14SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 14 CATCH BASIN

D-CB-16S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 16 CATCH BASIN

D-CB-17S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 17 CATCH BASIN

D-CB-25LP	02-20-20	LOW PROFILE 32" X 32" SQUARE CONCRETE NO. 25LP CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-26P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 26 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-26S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 26 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-27S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 27 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-31R	02-20-20	STANDARD PRECAST CIRCULAR NO. 31 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-31SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 31 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-31SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 31 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-32LP	02-20-20	STANDARD 80” X 32” RECTANGULAR CONCRETE NO. 32 CATCH BASIN (FOR USE UNDER CONCRETE MEDIUM BARRIER WALL)

D-CB-38RB	03-04-21	STANDARD PRECAST CIRCULAR NO. 38 CATCH BASIN

D-CB-38S	03-04-21	STANDARD 32" X 32" SQUARE CONCRETE NO. 38 CATCH BASIN

D-CB-38SB	03-04-21	STANDARD 4' X 4' SQUARE CONCRETE NO. 38 CATCH BASIN

D-CB-38SC	03-04-21	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 38 CATCH BASIN

D-CB-39RB	03-04-21	STANDARD PRECAST CIRCULAR NO. 39 CATCH BASIN

D-CB-39S	03-04-21	STANDARD 4' X 4' SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-39SC	03-04-21	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-39SD	03-04-21	STANDARD 7' X 7' SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-39SE	03-04-21	STANDARD 9' X 9' SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-40S	03-04-21	STANDARD 4' X 8' RECTANGULAR CONCRETE NO. 40 CATCH BASIN

D-CB-40SE	03-04-21	STANDARD 9’ X 9’ SQUARE CONCRETE NO. 40. CATCH BASIN

D-CB-41LP	02-20-20	LOW PROFILE 32" X 32" SQUARE CONCRETE NO. 41LP CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41P	02-20-20	STANDARD PRECAST 4' x 3' RECTANGULAR CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41S	02-20-20	STANDARD 4' X 3' RECTANGULAR CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-42RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 42 CATCH BASIN

D-CB-42S	02-20-20	STANDARD 32" X 32" SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-42SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-42SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-42SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-43R	02-20-20	STANDARD PRECAST CIRCULAR NO. 43R CATCH BASIN

D-CB-43SB	02-20-20	STANDARD 8' X 4' RECTANGULAR CONCRETE NO. 43SB CATCH BASIN

D-CB-43SC	02-20-20	STANDARD 8' X 5' 2" RECTANGULAR CONCRETE NO. 43SC CATCH BASIN

D-CB-44SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 44 CATCH BASIN

D-CB-45S	02-20-20	STANDARD 8' X 4' RECTANGULAR CONCRETE NO. 45 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-46SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 46 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-51SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 51 CATCH BASIN (FOR USE IN FRONT OF CONCRETE RETAINING WALL)

D-CB-51SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 51 CATCH BASIN (FOR USE IN FRONT OF CONCRETE RETAINING WALL)

D-CB-51SE	02-20-20	STANDARD 9’ X 9’ SQUARE CONCRETE NO. 51 CATCH BASIN

D-CB-52SE	02-20-20	STANDARD 9’ x 9’ SQUARE CONCRETE NO. 52 CATCH BASIN

D-CB-99	02-20-20	MISCELLANEOUS DETAILS FOR RECTANGULAR STRUCTURES

D-CB99-GS	CATCH BASIN DETAILS FOR GRADE SEPARATION WALL

D-CB-99R	01-28-22	MISCELLANEOUS DETAILS FOR ROUND STRUCTURES

D-CB-99RA	10-29-21	BILL OF STEEL FOR ROUND CATCH BASIN LIDS

D-CB-99RB	02-20-20	ROUND JUNCTION BOX SPRING DRAIN BOX

D-CBB-12A	06-28-19	TYPE ‘B’ CAST IRON FRAME, GRATE & VERTICAL INLET DETAILS FOR NOS. 10, 12, 14, 16 & 17 TYPE CATCH BASINS

D-CBB-12B	06-28-19	TYPE ‘B’ CAST IRON FRAME, GRATE & 6" SLOPING INLET DETAILS FOR NOS. 25, 26 & 27 TYPE CATCH BASINS

D-CBB-12D	07-07-23	TYPE "B" CAST IRON FRAME, GRATE & CURB HOOD DETAILS FOR NOS. 12, 14, 16 & 17 TYPE CATCH BASINS

D-CBB-13	06-28-19	TYPE ‘B’ CAST IRON FRAME, GRATE & VERTICAL INLET DETAILS FOR NO. 13 TYPE CATCH BASINS

D-CBB-31	02-20-20	TYPE “B” CAST IRON FRAME, GRATE & INLET DETAILS FOR NOS. 31, 41, 45, 46, & 51 TYPE CATCH BASINS

D-CBB-42	10-29-21	CAST IRON GRATE DETAILS FOR NOS. 42, 43 & 44 TYPE CATCH BASINS

D-RL-1	ROUND LID DETAILS FOR SINGLE CURB AND WALL INLET

D-RL-2	ROUND LID DETAILS FOR DOUBLE CURB AND WALL INLET

D-RL-3	ROUND LID DETAILS FOR SINGLE OPENING AREA DRAIN

D-RL-4	ROUND LID DETAILS FOR DOUBLE OPENING AREA DRAIN

D-RS-1	PRECAST ROUND STRUCTURES (48” THRU 120”)

D-RS-2	PRECAST ROUND STRUCTURES REINFORCEMENT DETAILS

D-RS-3	MISCELLANEOUS DETAILS FOR ROUND STRUCTURES

10-103.02	JUNCTION BOXES

D-JBS-1	02-20-20	STANDARD 32" X 32" SQUARE CONCRETE NO. 1 JUNCTION BOX

D-JBS-2	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 2 JUNCTION BOX

D-JBS-3	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 3 JUNCTION BOX

D-JBS-4	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 4 JUNCTION BOX

D-JBS-5	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 5 JUNCTION BOX

D-RJB-1	PRECAST ROUND JUNCTION BOX STRUCTURES (48” THRU 120”)

10-103.03	MANHOLES

D-MH-2	02-20-20	STANDARD PRECAST NO. 3 MANHOLE

D-MH-3	02-20-20	TYPICAL DESIGN OF LIDS FOR NO. 3 MANHOLE

D-MH-4	02-20-20	STANDARD NO. 3 MANHOLE CASTINGS AND STEPS

D-MH-5	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 3 MANHOLE

D-MH-6	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 3 MANHOLE

D-MH-7	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 3 MANHOLE

D-RMH-1	PRECAST MANHOLE STRUCTURES (48” THRU 120”)

10-103.04	PRECAST RISERS

D-RF-1	07-30-24	STANDARD PRECAST RISER

10-103.05	SPRING DRAIN BOXES

D-SDS-1	02-20-20	STANDARD 32" X 32" SQUARE CONCRETE NO. 1 SPRING DRAIN BOX

D-SDS-2A	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 2A SPRING DRAIN BOX

D-SDS-2B	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 2B SPRING DRAIN BOX

D-SDS-3A	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 3A SPRING DRAIN BOX

D-RSB-1	PRECAST ROUND SPRING DRAIN BOX STRUCTURES (48” THRU 120”)

10-103.06	SLOTTED AND TRENCH DRAINS

D-SLD-1	02-20-20	SLOTTED DRAINS

D-SLD-2	02-20-20	SLOTTED DRAINS

D-SLD-3	02-20-20	SLOTTED DRAINS

D-TD-1	07-07-23	TRENCH DRAIN

10-104.00 ROADWAY, PAVEMENT APPURTENANCES, AND FENCES

10-104.01	CONCRETE PAVEMENT

RP-CS-1	05-01-20	CONCRETE SHOULDER RUMBLE STRIP DETAIL (FOR 4-LANE DIVIDED HIGHWAY)

RP-CS-2	05-01-20	CONCRETE SHOULDER RUMBLE STRIP DETAIL (FOR 6-LANE OR WIDER DIVIDED HIGHWAY)

RP-CS-3	CONCRETE SHOULDER MILLED RUMBLE STRIP DETAILS

RP-J-1	05-01-20	PORTLAND CEMENT CONCRETE PAVEMENT JOINT TYPES AND SPACING

RP-J-3	05-01-20	PORTLAND CEMENT CONCRETE PAVEMENT JOINT TYPES AND SPACING

RP-J-5	05-01-20	TYPICAL ACCELERATION AND DECELERATION LANE JOINT TYPES AND SPACING FOR CONCRETE RAMPS

RP-J-7	05-01-20	CONCRETE RAMP JOINT TYPES AND SPACING

RP-J-9	05-01-20	CONTRACTION AND CONSTRUCTION JOINTS FOR CONCRETE PAVEMENT

RP-J-11	05-01-20	3/4" AND 1 3/4" EXPANSION AND EDGE PAVEMENT JOINTS

RP-J-13	05-01-20	3/4" AND 1 3/4" ELASTOMERIC COMPRESSION JOINT SEALS

RP-J-15	05-01-20	LONGITUDINAL CONTRACTION AND CONSTRUCTION JOINTS

RP-J-17	05-01-20	DOWEL ASSEMBLY DEVICES

RP-J-18	01-28-22	DOWEL ASSEMBLY DEVICES

RP-J-19	05-01-20	DOWEL ASSEMBLY DEVICES

RP-J-23	01-28-22	CONCRETE PAVEMENT REPAIR DETAILS

RP-J-24	05-01-20	CONCRETE PAVEMENT SPALL AND RANDOM CRACK REPAIR DETAILS

RP-J-25	05-01-20	CONCRETE PAVEMENT JOINT REPAIR DETAILS

RP-EPO-1	EMERGENCY PULL OVER AREA

10-104.02	INTERSECTIONS

RP-D-15	04-01-25	DETAILS OF STANDARD CONCRETE DRIVEWAYS

RP-D-16	04-01-25	DETAILS OF LOWERED STANDARD CONCRETE DRIVEWAYS

RP-DHO-1	05-01-20	MEDIAN OPENINGS ON 4-LANE DIVIDED HIGHWAY

RP-DHO-2	07-30-24	MEDIAN OPENING DETAILS FOR RESTRICTED CROSSING & J-TURN INTERSECTIONS

RP-I-5	05-01-20	EXAMPLES OF STREET & ALLEY INTERSECTIONS

RP-PMR-1	05-01-20	STANDARD DETAILS FOR PROPOSED PERMANENT MAINTENANCE RAMP

RP-R-1	04-21-25	STANDARD RAMP DETAILS FOR ROADWAYS AND DRIVEWAYS

RP-R-1A	04-21-25	STANDARD RAMP DETAILS FOR LOW VOLUME RURAL ROADWAYS

10-104.03	CURBS

RP-SC-1	05-04-22	SLOPING CONCRETE CURB AND CURB AND GUTTER

RP-VC-10	03-04-21	VERTICAL CONCRETE CURB AND CURB AND GUTTER (FOR 8” TO 12” GUTTER DEPTH)

RP-VC-11	03-04-21	VERTICAL CONCRETE CURB AND CURB AND GUTTER (FOR 6” & 7” GUTTER DEPTH)

10-104.04	WALLS

W-CIP-1	05-01-20	ROADWAY FEATURES AT CAST IN PLACE RETAINING WALL

W-MSE-1	05-01-20	ROADWAY FEATURES FOR MSE SEGMENTAL PRECAST FACING RETAINING WALL

W-MSE-2	05-01-20	ROADWAY FEATURES FOR MSE MODULAR BLOCK FACING RETAINING WALL

W-SG-1	07-30-24	STANDARD GRAVITY-TYPE RETAINING WALLS

W-SP-1	05-01-20	ROADWAY FEATURES AT SOLDIER PILE AND SOIL ANCHORED RETAINING WALLS

10-104.05	FENCES AND RIGHT-OF-WAY MARKERS

S-F-1	03-01-23	HIGH VISIBILITY FENCE

S-F-10	07-17-20	STANDARD RIGHT-OF-WAY STOCK FENCE

S-F-10A	06-28-19	STANDARD RIGHT-OF-WAY STOCK FENCE WITH TIMBER POSTS

S-F-10B	06-28-19	STANDARD RIGHT-OF-WAY CHAIN LINK FENCE

S-F-10C	06-28-19	RIGHT-OF-WAY FENCE AT BRIDGES AND BOX CULVERTS

S-F-10D	06-28-19	RIGHT-OF-WAY FENCE LOCATIONS AT INTERCHANGES

S-FG-11	07-30-24	STOCK FENCE GATES AND CHAIN LINK FENCE CLOSURE

S-FG-20	06-28-19	EXAMPLES OF WATER GATES AND WATER CROSSINGS

S-RP-2	06-28-19	STANDARD CONCRETE RIGHT-OF-WAY MARKERS

10-105.00 MULTIMODAL

10-105.01	CURB RAMPS

CR-GN-1	GENERAL NOTES CURB RAMP

CR- GN-2	CURB RAMP NUMBERING

CR-DWS-1	DETECTABLE WARNING SURFACE DETAIL

CR-PLL-1	PUSH BUTTON LOCATION LAYOUT

CR-CRT-1	CURB RAMP TYPES

CR-GTL-1	GUTTER TRANSITION LAYOUT

CR-GT-2	GUTTER TRANSITION LAYOUT

CR-PL-1	PERPENDICULAR CURB RAMP PLACEMENT LAYOUT

CR-10	PERPENDICULAR CURB RAMP

CR-11	PERPENDICULAR CURB RAMP WITH BRICK DETAILS

CR-PL-2	PARALLEL CURB RAMP PLACEMENT LAYOUT

CR-20	PARALLEL CURB RAMP 5 – FT SIDEWALK

CR-21	COMBINATION RAMP USED WITH WIDE SIDEWALK

CR-22	COMBINATION CURB RAMP

CR-23	PARALLEL CURB RAMP WITH EXISTING BRICK

CR-30	CURB RAMPS IN CURVE BI-DIRECTIONAL DUAL CROSSING

CR-31	BLENDED TRANSITION BI-DIRECTIONAL

CR-32	LOWERED CORNER RAMP

CR-33	SINGLE CROSSING CURB RAMP IN CURVE

CR-34	SINGLE CROSSING CURB RAMP IN CURVE

CR-40	MONO-DIRECTIONAL SINGLE CROSSWALK CURB RAMP DETAILS

CR-41	SINGLE CROSSING CURB RAMP IN CURVE

CR-50	PEDESTRIAN REFUGE

CR-51	PEDESTRIAN REFUGE

10-105.02	PAVEMENT MARKING

MM-PM-1	SIGNING AND PAVEMENT MARKINGS AT INTERSECTION CROSSINGS FOR SHARED-USE PATHS

MM-PM-2	07-30-24	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANE OR ROUTES

MM-PM-3	06-15-21	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANES ON URBAN ROADWAYS

MM-PM-4	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANES

MM-PM-5	05-04-22	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANES AT INTERSECTIONS

10-105.03	SAFETY RAIL

MM-BPR-1	03-21-25	BIKE AND PEDESTRIAN SAFETY RAIL

MM-BPR-2	10-16-20	BIKE AND PEDESTRIAN MEDIAN BARRIER RAIL

MM-BPR-3	03-24-25	32 INCH HALF SIZE SINGLE SLOPE BARRIER WALL & SLOPED END TREATMENT.

MM-VPR-1	VEHICLE AND PEDESTRIAN SAFETY RAIL

10-105.04	SIDEWALK

MM-PS-1	DETAILS FOR PEDESTRIAN STEPS AND HANDRAILS

MM-SW-1	07-07-23	DETAILS FOR CONCRETE SIDEWALKS

MM-SW-2	ALTERNATE DETAILS FOR CONCRETE SIDEWALK (REHABILITATION)

10-105.05	TYPICAL SECTION

MM-BS-1	TYPICAL BUS STOP LOCATION

MM-TS-1	06-15-21	BIKE ACCOMMODATION DESIGN GUIDANCE

MM-TS-2	06-15-21	LATERAL OFFSETS FOR SIDEWALK AND SHARED USE PATH

MM-TS-3	07-30-24	SEPARATED SHARED USE PATH TYPICAL SECTIONS

MM-PM-3	06-15-21	SIGNING AND PAVEMENT MARKING FOR BIKE LANES ON URBAN ROADWAYS

10-106.00 SAFETY DESIGN AND GUARDRAILS

10-106.01	CLEAR ZONE AND SAFETY PLANS

S-CZ-1	06-28-19	CLEAR ZONE CRITERIA

S-PL-1	03-01-23	SAFETY PLAN FOR BARRIER LENGTH OF NEED

S-PL-1A	03-01-23	SAFETY PLAN FOR BARRIER LENGTH OF NEED (FOR RIGID OBJECTS)

S-PL-1B	03-01-23	SAFETY PLAN FOR BARRIER LENGTH OF NEED ON CURVED ROADWAYS

S-PL-3	03-01-23	SAFETY PLAN MINIMUM INSTALLATION AT BRIDGE ENDS

S-PL-4	01-09-24	SAFETY PLAN FOR BRIDGE PIERS IN DEPRESSED MEDIAN

S-PL-4A	01-09-24	SAFETY PLAN TO FOR BRIDGE PIERS/ ABUTMENTS OUTSIDE THE SHOULDER

S-PL-5	06-28-19	SAFETY PLAN FOR BRIDGE ENDS IN MEDIANS

S-PL-6	07-30-24	SAFETY PLAN SAFETY HARDWARE PLACEMENT ON OUTSIDE EDGE

S-PL-6A	06-28-19	SAFETY PLAN SAFETY HARDWARE PLACEMENT IN MEDIAN

S-PL-7	SAFETY PLAN HARDWARE PLACEMENT AT INTERSECTIONS

10-106.02	CABLE BARRIER

S-CB-1	01-09-24	CABLE BARRIER PLACEMENT

S-CB-2	07-07-23	HIGH TENSION CABLE BARRIER

10-106.03	CRASH CUSHIONS

S-CC-1	10-01-24	CRASH CUSHION

S-CC-2	06-28-19	CRASH CUSHION (GATING) BARREL ARRAY

10-106.04	GUARDRAIL DETAILS

S-GR31-1	03-13-25	GUARDRAIL DETAILS

S-GR31-1A	06-28-19	GUARDRAIL AND BLOCK-OUT DETAILS

S-GR31-1B	GUARDRAIL FASTENING HARDWARE

S-GR31-1C	07-07-23	GUARDRAIL GENERAL NOTES AND POST DETAILS

S-GR1-1D	03-01-23	GUARDRAIL POST PLACEMENT IN ROCK

10-106.05	GUARDRAIL CONNECTIONS

S-AGT-1	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-AGT-2	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-AGT-3	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-AGT-4	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-AGT-5	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-AGT-6	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-AGT-7	LONG SPAN APPROACH GUARDRAIL TRANSITION

S-GRC-4	01-30-25	GUARDRAIL CONNECTION TO BRIDGE RAILING CONCRETE PARAPET

S-GRC-5	02-28-20	GUARDRAIL CONNECTION TO BRIDGE ENDS (TRAILING ENDS)

S-GRC-6	07-07-23	GUARDRAIL CONNECTION TO BRIDGE ENDS FOR LOW SPEED ROADWAYS

10-106.06	GUARDRAIL (SPECIAL CASES)

S-CPW-1	CURVED PARAPET WALL ≤ 40 M.P.H.

S-GRS-1	06-15-21	SPECIAL CASE LONG SPAN GUARDRAIL 1 POST, 2 OR 3 POSTS OMITTED

S-GRS-2	01-28-22	SPECIAL CASE GUARDRAIL ATTACHMENT TO CONCRETE DECKS

S-GRS-3	06-28-19	SPECIAL CASE GUARDRAIL FOOTING

S-GRS-4	05-04-22	SPECIAL CASE GUARDRAIL HEIGHT TRANSITION DETAIL

S-GRS-5	SPECIAL CASE WEAK-POST GUARDRAIL ATTACHMENT TO CULVERT

S-GRS-5A	06-15-21	WEAK-POST GUARDRAIL ASSEMBLY DETAILS FOR TYPE 1 & 2

S-GRS-5B	WEAK-POST GUARDRAIL ASSEMBLY DETAILS FOR TYPE 3 & 4

S-GRS-6	01-30-25	SPECIAL CASE FLEXIBITLTY ON GUARDRAIL POST INSTALLATIONS

S-GRS-7	01-09-24	SHORT RADIUS-GR SYSTEM (SRGS) CONNECTION TO BRIDGE END

S-GRS-7A	07-30-24	SHORT RADIUS-GUARDRAIL SYSTEM (SRGS) ANCHOR DETAILS

S-GRS-7B	SHORT RADIUS-GR SYSTEM (SRGS) EYE-BOLT SPACING DETAILS

S-GRS-8 SAFETY PLAN AT SIDEROADS OR DRIVEWAYS FOR LOW

SPEED ROADWAYS

10-106.07	GUARDRAIL TERMINALS

S-GRT-1	10-29-21	TYPE 12 GUARDRAIL TERMINAL BURIED-IN-BACKSLOPE

S-GRT-1A	LAYOUT OF FLARED GUARDRAIL (TL- 3)

S-GRT-1B	LAYOUT OF FLARED GUARDRAIL (TL- 2)

S-GRT-2	06-28-19	TYPE 38 GUARDRAIL END TERMINAL

S-GRT-2P	10-16-20	EARTH PAD FOR TYPE 38 AND TYPE 21 TERMINAL

S-GRT-2R	06-28-19	EARTH PAD FOR TYPE 38 AND TYPE 21 TERMINAL (RETROFIT)

S-GRT-3	06-28-19	TYPE 21 GUARDRAIL END TERMINAL

S-GRT-4	01-30-25	TYPE 21 GATING END TERMINAL

S-GRT-4A	TYPE 21 GATING END TERMINAL ANCHOR DETAILS

S-GRT-4B	GATING TERMINAL POST & RAIL DETAILS

10-106.08	GUARDRAIL ANCHORS

S-GRA-1	06-28-19	TYPE 12 GUARDRAIL ANCHOR

S-GRA-1A	06-28-19	GUARDRAIL ANCHOR FOR TYPE 12 TERMINAL (ALTERNATIVE)

S-GRA-3	01-09-24	TYPE 13 GUARDRAIL ANCHOR

S-GRA-4	03-01-23	IN-LINE GUARDRAIL ANCHOR TO PRIVATE DRIVE

S-GRA-5	06-28-19	FLARED GUARDRAIL ANCHOR

10-106.09	CONCRETE MEDIAN BARRIERS

S-SSMB-1	01-28-22	32” SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-1A	10-29-21	36” SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-2	10-29-21	51” SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-3	10-29-21	51” HALF SIZE SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-4	07-17-20	FLARED SINGLE SLOPE CONCRETE MEDIAN BARRIER WALL (VERTICAL BACK)

S-SSMB-5	05-01-20	SINGLE SLOPE MEDIAN BARRIER WALL CATCH BASIN DETAIL

S-SSMB-6	06-28-19	32"CONCRETE SINGLE SLOPE BARRIER WALL WITH SINGLE GUARDRAIL ATTACHMENT

S-SSMB-6A	36” CONCRETE SINGLE SLOPE BARRIER WALL FOR ATTACHING GUARDRAIL

S-SSMB-6B	DUAL GUARDRAIL ATTACHMENT TO SINGLE SLOPE 36” BARRIER WALL

S-SSMB-6C	SINGLE GUARDRAIL ATTACHMENT TO SINGLE SLOPE 36” BARRIER WALL

S-SSMB-6D	51” CONCRETE SINGLE SLOPE BARRIER WALL FOR ATTACHING GUARDRAIL

S-SSMB-6E	DUAL GUARDRAIL ATTACHMENT TO SINGLE SLOPE 51” BARRIER WALL

S-SSMB-6F	SINGLE GUARDRAIL ATTACHMENT TO SINGLE SLOPE 51” BARRIER WALL

S-SSMB-7	05-01-20	FOOTING DETAILS FOR OVERHEAD SIGN STRUCTURE 32” MEDIAN BARRIER WALL

S-SSMB-8	05-01-20	FOOTING DETAILS FOR OVERHEAD SIGN STRUCTURE 51” MEDIAN BARRIER WALL

S-SSMB-9	10-29-21	SINGLE SLOPE BARRIER WALL FOR GRADE SEPARATED MEDIAN

S-SSMB-10	01-09-24	SPECIAL DETAIL FOR CONCRETE MEDIAN BARRIER WALL TRANSITION FROM 32” TO 51”

10-106.10	GUARDRAIL MAINTENANCE

S-GR28-1M	06-15-21	W-BEAM & THRIE BEAM BARRIER RAIL AND RUB RAIL DETAILS

S-GR28-2M	06-28-19	GUARDRAIL HARDWARE DETAILS

S-GR28-3M	01-28-22	GUARDRAIL HEIGHT ADJUSTMENT

S-GR28-4M	06-28-19	GUARDRAIL TERMINAL ANCHOR TYPE 13

S-GR28-5M	06-28-19	MEDIAN DIVIDER GUARDRAIL

S-GR28-6M	10-29-21	GUARDRAIL ATTACHMENT TO CONCRETE DECKS

S-GR28-7M	06-28-19	GUARDRAIL ATTACHMENT TO BRIDGE END DETAILS MAINTENANCE ONLY

S-GRC-1M	GUARDRAIL CONNECTION TO BRIDGE ENDS OR BARRIER WALL

S-GRC-2M	GUARDRAIL CONNECTION TO BRIDGE END FOR LOCAL ROADS (ADT<2000)

S-GRC-3M	MEDIAN DIVIDER GUARDRAIL TRANSITION TO CONCRETE MEDIAN BARRIER

S-PL-2M	SAFETY PLAN AT SIDE ROADS OR PRIVATE DRIVES

S-SSMB-6M	GUARDRAIL ATTACHMENT TO EXISTING SINGLE SLOPE CONCRETE BARRIER WALL

10-107.00 EROSION PREVENTION AND SEDIMENT CONTROL

10-107.01	DEWATERING DEVICES

EC-STR-1	08-01-12	DEWATERING STRUCTURE

EC-STR-2	08-01-12	SEDIMENT FILTER BAG

10-107.02	SLOPE DEVICES

EC-STR-3B	06-15-21	SILT FENCE

EC-STR-3C	03-01-23	SILT FENCE WITH WIRE BACKING

EC-STR-3D	03-01-23	ENHANCED SILT FENCE

EC-STR-3E	04-01-08	SILT FENCE FABRIC JOINING DETAILS

EC-STR-8	06-10-14	FILTER SOCK

EC-STR-27	08-01-12	TEMPORARY SLOPE DRAIN AND BERM

EC-STR-29	08-01-12	PERMANENT SLOPE DRAIN PIPE

EC-STR-34	05-04-22	EROSION CONTROL BLANKET FOR SLOPE INSTALLATION

EC-STR-35	08-01-12	FILTER BERMS

EC-STR-37	06-10-14	SEDIMENT TUBE

10-107.03	DITCH DEVICES

EC-STR-4	07-30-24	ENHANCED SILT FENCE CHECK (TRAPEZOIDAL DITCH)

EC-STR-4A	07-30-24	ENHANCED SILT FENCE CHECK (V-DITCH)

EC-STR-4B	08-01-12	ENHANCED SILT FENCE CHECK DETAILS

EC-STR-6	11-30-20	ROCK CHECK DAM

EC-STR-6A	05-06-16	ENHANCED ROCK CHECK DAM

EC-STR-7	05-04-22	SEDIMENT TRAP WITH CHECK DAM

EC-STR-55	08-01-12	GABION CHECK DAM

EC-STR-56	04-01-08	GABION CHECK DAM DESIGN TABLES

EC-STR-57	04-01-08	GABION ASSEMBLY DETAILS

EC-STR-58	04-01-08	GABION ASSEMBLY DETAILS

EC-STR-59	08-01-12	GABION CHECK DAM GENERAL NOTES AND COMPONENT PROPERTIES

EC-STR-61	03-16-17	LEVEL SPREADERS

10-107.04	INLET PROTECTION

EC-STR-11	03-16-17	CULVERT PROTECTION TYPE 1

EC-STR-19	04-01-08	CATCH BASIN PROTECTION

EC-STR-39	08-01-12	CURB INLET PROTECTION TYPE 1 & 2

EC-STR-39A	08-01-12	CURB INLET PROTECTION TYPE 3 & 4

EC-STR-40	CATCH BASIN FILTER ASSEMBLY FOR CIRCULAR STRUCTURES

EC-STR-41	CATCH BASIN FILTER ASSEMBLY (TYPE 1)

EC-STR-41A	CATCH BASIN FILTER ASSEMBLY (TYPE 1) SLIPCOVER DETAILS

EC-STR-42	CATCH BASIN FILTER ASSEMBLY (TYPE 2)

EC-STR-42A	CATCH BASIN FILTER ASSEMBLY (TYPE 2) SLIPCOVER DETAILS

EC-STR-43	CATCH BASIN FILTER ASSEMBLY (TYPE 3)

EC-STR-43A	CATCH BASIN FILTER ASSEMBLY (TYPE 3) SLIPCOVER DETAILS

EC-STR-44	CATCH BASIN FILTER ASSEMBLY (TYPE 4)

EC-STR-44A	CATCH BASIN FILTER ASSEMBLY (TYPE 4) SLIPCOVER DETAILS

EC-STR-45	CATCH BASIN FILTER ASSEMBLY (TYPE 5)

EC-STR-45A	CATCH BASIN FILTER ASSEMBLY (TYPE 5) SLIPCOVER DETAILS

EC-STR-46	CATCH BASIN FILTER ASSEMBLY (TYPE 6)

EC-STR-46A	CATCH BASIN FILTER ASSEMBLY (TYPE 6) SLIPCOVER DETAILS

EC-STR-47	CATCH BASIN FILTER ASSEMBLY (TYPE 7)

EC-STR-47A	CATCH BASIN FILTER ASSEMBLY (TYPE 7) SLIPCOVER DETAILS

EC-STR-48	CATCH BASIN FILTER ASSEMBLY (TYPE 8)

EC-STR-48A	CATCH BASIN FILTER ASSEMBLY (TYPE 8) SLIPCOVER DETAILS

EC-STR-49	CATCH BASIN FILTER ASSEMBLY (TYPE 9)

EC-STR-49A	CATCH BASIN FILTER ASSEMBLY (TYPE 9) SLIPCOVER DETAILS

EC-STR-50	CATCH BASIN FILTER ASSEMBLY (TYPE 10)

EC-STR-50A	CATCH BASIN FILTER ASSEMBLY (TYPE 10) SLIPCOVER DETAILS

EC-STR-51	CATCH BASIN FILTER ASSEMBLY (TYPE 11)

EC-STR-51A	CATCH BASIN FILTER ASSEMBLY (TYPE 11) SLIPCOVER DETAILS

10-107.05	DETAINING DEVICES

EC-STR-12	08-01-12	ROCK SEDIMENT DAM

EC-STR-13	08-01-12	ROCK AND EARTH SEDIMENT EMBANKMENT

EC-STR-15	08-01-12	SEDIMENT BASIN

EC-STR-16	08-01-12	SEDIMENT BASIN RISER AND COLLAR APPURTENANCES

EC-STR-17	08-01-12	SEDIMENT BASIN EMBANKMENT DETAILS

EC-STR-18	SEDIMENT BASIN FLOATING OUTLET STRUCTURE

EC-STR-21	05-04-22	PERMANENT RIPRAP BASIN ENERGY DISSIPATORS

10-107.06	IN-STREAM DEVICES

EC-STR-11A	08-01-12	CULVERT PROTECTION TYPE 2

EC-STR-25	08-01-12	TEMPORARY CULVERT CROSSING, CONSTRUCTION EXIT, CONSTRUCTION FORD

EC-STR-30	INSTREAM DIVERSION (WITHOUT TRAFFIC)

EC-STR-30A	INSTREAM DIVERSION (WITH TRAFFIC)

EC-STR-31	05-04-22	TEMPORARY DIVERSION CHANNEL

EC-STR-31A	04-01-08	TEMPORARY DIVERSION CHANNEL DESIGN

EC-STR-32	08-01-12	TEMPORARY DIVERSION CULVERTS

EC-STR-33	08-01-12	SUSPENDED PIPE DIVERSION (DOWNSTREAM)

EC-STR-33A	08-01-12	SUSPENDED PIPE DIVERSION (UPSTREAM)

EC-STR-36	05-04-22	TURF REINFORCEMENT MAT FOR CHANNEL INSTALLATION

EC-STR-38	08-01-12	FLOATING TURBIDITY CURTAIN

10-108.00 NATURAL STREAM DESIGN

10-108.01	DEFLECTORS, VANES AND ENERGY DISSIPATORS

D-NSD-13	05-01-20	LONGITUDINAL STONE TOE

D-NSD-21	05-01-20	BOULDER CLUSTERS

D-NSD-22	05-01-20	BOULDER CROSS VANE

D-NSD-23	05-01-20	BOULDER CROSS VANE WITH STEP

D-NSD-24	05-01-20	BOULDER W-WEIR

D-NSD-25	05-01-20	BOULDER VANES AND J-HOOK

D-NSD-26	11-30-20	LOG VANES, ROOT WADS, AND BOULDER J-HOOK

D-NSD-27	11-30-20	LOG AND BOULDER STEP POOLS

D-NSD-28	05-01-20	BOULDER RIFFLES

D-NSD-28A	11-30-20	LOG RIFFLES

D-NSD-29	05-01-20	CONSTRUCTED ALLUVIAL RIFFLE

D-NSD-30	05-01-20	SUBSTRATE RESTORATION

D-NSD-31	05-01-20	CLAY CHANNEL PLUG

D-NSD-32	05-01-20	WOOD TOE WITH GEO-LIFTS

D-NSD-32A	05-01-20	BOULDER TOE WITH GEO-LIFTS

D-NSD-33	05-01-20	COIR FIBER EROSION CONTROL BLANKET AND

COIR FIBER ROLLS

D-NSD-34	05-01-20	LIVE STAKES AND LIVE SILTATION

D-NSD-35	05-01-20	LIVE FASCINES

D-NSD-36	05-01-20	BRUSH MATTRESS

D-NSD-37	05-01-20	SPECIAL NOTES FOR NATURAL STREAM DESIGN