ROADWAY INDEX	STANDARD ROADWAY DRAWINGS

❶SHEET NAME	SHEET NO.

DWG.	REV.	DESCRIPTION

DWG.	REV.	DESCRIPTION

SIGNATURE SHEETS	ROADWAY-SIGN1

TITLE SHEET	1

❷ROADWAY INDEX AND STANDARD ROADWAY DRAWINGS	1A

❷STANDARD ROADWAY DRAWINGS	1A1, 1A2

❷ STANDARD STRUCTURE AND TRAFFIC OPERATIONS DRAWINGS	1A3

PROJECT COMMITMENTS	1B

❸ESTIMATED ROADWAY QUANTITIES	2, 2-1, 2-2

❹ESTIMATED BOX BRIDGE QUANTITIES	2A, 2A1

❺TYPICAL SECTIONS AND PAVEMENT SCHEDULE	2B, 2B1, 2B2

GENERAL NOTES	2C, 2C1

SPECIAL NOTES	2D, 2D1

ENVIRONMENTAL NOTES	2E, 2E1

TABULATED QUANTITIES	2F, 2F1

DETAIL SHEETS	2G, 2G1, 2G2

RIGHT-OF-WAY NOTES, UTILITY NOTES, AND UTILITY OWNERS	3

PROPERTY MAP(S) AND RIGHT-OF-WAY ACQUISITION TABLE(S)	3A – 3B

PRESENT LAYOUT(S)	4 – 10

RIGHT-OF-WAY DETAILS	4A – 10A

PROPOSED LAYOUT(S)	4B – 10B

PROPOSED PROFILE(S)	4C – 10C

RAMP PROFILE(S)	11 – 12

SIDE ROADS PROFILE(S) ①	13 – 14

PRIVATE DRIVE, BUSINESS, AND FIELD ENTRANCE PROFILE(S)	15 – 18

DRAINAGE MAP(S)	19 – 20

CULVERT SECTION(S)	21 – 22

❻EROSION PREVENTION AND SEDIMENT CONTROL PLANS	23, 24, 25-27Z

ENVIRONMENTAL MITIGATION PLAN(S)	28, 28A, 28B

SIGNING AND PAVEMENT MARKING PLAN(S)	29 – 35

SIGN SCHEDULE SHEET(S)	36 – 39

❽MISCELLANEOUS SIGNING DETAILS	40 – 40Z

❾ROADWAY CROSS SECTIONS	41 – 95

❾SIDE ROAD CROSS SECTIONS	96 – 106

❼TRAFFIC CONTROL PLANS	T1 – T50Z

❼❿BRIDGE PLANS ……………………………………………………………B-1

❼❿GEOTECHNICAL PLANS	G-1

❼ITS PLANS	ITS-1

❼LIGHTING PLANS	L-1

❼❿NATURAL STREAM DESIGN PLANS	NS-1

❼⓫RETAINING WALL PLANS	R-1

❼SIGNAL PLANS	SIG-1

❼❿STORM WATER POLLUTION PREVENTION PLAN (SWPPP) PLANS	S-1

❼UTILITIES PLANS	U1–1

NOTE:	THE ALPHABETICAL LETTERS “I”, “O” & “Q” ARE NOT USED IN THE NUMBERING OF SHEETS.

Footnotes: (ADD IF NEEDED)

①	Haul Road profiles follow Side Road profiles in the sheet numbering sequence.

INDEX NOTES:

❶	THIS IS THE ORDER OF SHEETS THAT ALL ROADWAY CONSTRUCTION PLANS SHOULD BE SETUP. THE SHEET NAME IN THE INDEX OF SHEETS MUST MATCH EXACTLY WITH THE NAME ON THE PLAN SHEETS, IN THE SHEET TITLE BLOCK, IN THE LOWER RIGHT CORNER OF EACH SHEET.

IF ANY OF THE 2A THRU 2G SHEET SERIES ARE NOT USED, DO NOT RENUMBER THE SHEET SERIES SO THAT THE NUMBERING IS CONSECUTIVE. KEEP THE SHEET SERIES NUMBER AS A PLACEHOLDER SO THAT IT CAN BE ADDED TO THE INDEX LATER IF NEEDED. THE INDEX SHOULD NEVER GO PAST SHEET 2G IN THE SECOND SHEET UNLESS THERE IS A SPECIAL CIRCUMSTANCE.

❷	THE ROADWAY INDEX AND STANDARD ROADWAY DRAWINGS WILL HAVE THE SAME SHEET NUMBERING SERIES 1A, 1A1, 1A2, ETC. THERE SHOULD BE NO NEED TO CUT AND PASTE BETWEEN SHEETS. STANDARD TRAFFIC OPERATIONS & STRUCTURE DRAWINGS SHOULD BE ON THEIR SHEET.

❸	THE ESTIMATED ROADWAY QUANTITIES BLOCK(S) ARE NUMBERED 2, 2-1, 2-2, ETC. THIS SERIES OF SHEETS CAN BE ADJUSTED ACCORDING TO WHAT SHEETS YOU HAVE. EXAMPLE: IF YOU ONLY HAVE ONE SHEET OF ESTIMATED ROADWAY QUANTITIES, ITS SHEET NUMBER WOULD BE 2.

❹	THE ESTIMATED BOX BRIDGE QUANTITIES ARE NUMBERED SERIES 2A AND 2A1 FOR A SECOND SHEET.

❺	IF THE DGN SHEET ONLY HAS TYPICAL SECTIONS ON IT;

THEN THE NAME ON THE SHEET, IN THE SHEET TITLE BLOCK, IN THE LOWER RIGHT CORNER MUST BE “TYPICAL SECTIONS”.

IF THE DGN SHEET HAS TYPICAL SECTIONS AND THE PAVING SCHEDULE;

THEN THE NAME ON THE SHEET, IN THE SHEET TITLE BLOCK, IN THE LOWER RIGHT CORNER MUST BE “TYPICAL SECTIONS AND PAVEMENT SCHEDULE”.

❻	EACH STAGE OF EROSION CONTROL SHALL CORRESPOND WITH THE TRAFFIC CONTROL PHASE. EROSION PREVENTION AND SEDIMENT CONTROL PLANS SHALL BE LISTED AS EROSION PREVENTION AND SEDIMENT CONTROL PLANS IN THE INDEX. HOWEVER, WITHIN THE PLAN SET, THE FOLLOWING SHALL BE THE ORDER:

23. EPSC SPECIAL NOTES

24. EPSC LEGEND AND TABULATION

25-27Z. EPSC PLAN SHEETS (THIS REPRESENTS THREE STAGES OF EROSION CONTROL; 25, 25A, ETC., 26, 26A ETC. 27, 27A, ETC.)

❼	TRAFFIC, BRIDGE, GEOTECHNICAL, ITS, LIGHTING, NATURAL STREAM DESIGN, RETAINING, SIGNAL, SWPPP, AND UTILITY PLANS DIFFER FROM EACH OTHER AND HAVE THEIR NUMBERING SERIES AS SHOWN.

❽	EXAMPLE FOR NUMBERING AS SHOWN:

SHEET NO’S. xx, xxA, xxB, xxC THRU xxZ, ETC.

❾	EACH CROSS-SECTION SHEET MUST BE LABELED WITH THE NAME OF THE ROADWAY AS SHOWN ON THE PRESENT AND PROPOSED LAYOUT SHEETS IN THE BOTTOM RIGHT CORNER OF THE CROSS SECTIONS.

❿	SHEET NUMBERING EXAMPLES FOR BRIDGE, GEOTECHNICAL, NATURAL STREAM DESIGN, ANDSTORMWATER POLLUTION PREVENTION PLAN: G-1, G-2. G-3, ETC., NS-1, NS-2, NS-3 ETC.

⓫	SHEET NUMBERING EXAMPLE:

R, RA, RB, Etc.	(Estimated Quantities and Details) (All Walls)

Retaining Wall R-1	(Geotechnical Design Notes and Requirements),

Retaining Wall R-1A	(Geometric Layout)

Retaining Wall R-1B	(Soil Profiles and Details)

Retaining Wall R-1C	(If Needed)

Retaining Wall R-2	(Geotechnical Design Notes and Requirements),

Retaining Wall R-2A	(Geometric Layout)

Retaining Wall R-2B	(Soil Profiles and Details)

Retaining Wall R-2C	(If Needed)

Etc. For Each Wall

10-100.00 STANDARD ROADWAY TITLE SHEET, ABBREVIATIONS, AND LEGENDS

10-100.01	STANDARD ROADWAY DRAWINGS TITLE SHEET

RD-TP-1	09-26-16	STANDARD ROADWAY DRAWINGS TITLE SHEET

10-100.02	STANDARD ABBREVIATIONS AND LEGENDS

RD-A-1	02-20-20	STANDARD ABBREVIATIONS A THROUGH L

RD-A-2	STANDARD ABBREVIATIONS M THROUGH Z

RD-L-1	02-20-20	STANDARD LEGEND

RD-L-1A	STANDARD LEGEND

RD-L-2	02-20-20	STANDARD LEGEND FOR UTILITY INSTALLATIONS

RD-L-3	03-01-23	STANDARD LEGEND FOR SIGNALIZATION AND LIGHTING

RD-L-4	02-20-20	STANDARD LEGEND FOR SIGNALIZATION AND LIGHTING

RD-L-5	02-20-20	STANDARD LEGEND FOR EROSION PREVENTION AND SEDIMENT CONTROL

RD-L-6	02-20-20	STANDARD LEGEND FOR EROSION PREVENTION AND SEDIMENT CONTROL

RD-L-7	02-20-20	STANDARD LEGEND FOR EROSION PREVENTION AND SEDIMENT CONTROL

RD-L-8	02-20-20	STANDARD LEGEND FOR NATURAL STREAM DESIGN

10-101.00 ROADWAY DESIGN STANDARDS

10-101.01	RD18 TYPICAL SECTIONS AND DESIGN CRITERIA

RD18-RTS-1	DESIGN STANDARDS FOR SINGLE LANE URBAN AND RURAL ROUNDABOUTS

RD18-RTS-2	DESIGN STANDARDS FOR MULTI-LANE URBAN AND RURAL ROUNDABOUTS

RD18-RTS-3	STANDARD CONSTRUCTION DETAILS FOR ROUNDABOUTS

RD18-RSD-1	SIGHT DISTANCE FOR URBAN AND RURAL ROUNDABOUT

10-101.02	RD11 TYPICAL SECTIONS AND DESIGN CRITERIA

RD11-SE-1	TRANSITION AND CROSS SLOPE DETAILS

RD11-SE-2	SUPERELEVATION TRANSITION DETAILS FOR UNDIVIDED ROADWAYS

RD11-SE-2A	SUPERELEVATION TRANSITION SECTIONS FOR UNDIVIDED ROADWAYS

RD11-SE-3	SUPERELEVATION TRANSITION DETAILS FOR DIVIDED ROADWAYS

RD11-SE-3A	SUPERELEVATION TRANSITION SECTIONS FOR DIVIDED ROADWAYS

RD11-TS-1	06-28-19	DESIGN STANDARDS FOR LOW-VOLUME ROADS

RD11-TS-1A	06-28-19	DESIGN STANDARDS FOR LOCAL ROADS AND STREETS

RD11-TS-2	DESIGN STANDARDS FOR COLLECTORS, 2-LANE ROADS AND STREETS

RD11-TS-2A	DESIGN STANDARDS FOR COLLECTOR HIGHWAYS WITH DEPRESSED MEDIAN (4 AND 6 LANE)

RD11-TS-2B	DESIGN STANDARDS FOR COLLECTOR HIGHWAYS WITH FLUSH MEDIAN (4 AND 6 LANE)

RD11-TS-3	DESIGN STANDARD FOR ARTERIAL HIGHWAYS (2-LANE)

RD11-TS-3A	06-28-19	DESIGN STANDARDS FOR ARTERIAL HIGHWAYS WITH DEPRESSED MEDIAN (4 AND 6 LANE)

RD11-TS-3B	DESIGN STANDARDS FOR ARTERIAL HIGHWAYS WITH FLUSH MEDIAN (4 AND 6 LANE)

RD11-TS-3C	DESIGN STANDARDS FOR ARTERIALS WITH INDEPENDENT ROADWAYS (4 AND 6 LANE)

RD11-TS-4	DESIGN STANDARDS FOR ARTERIAL AND FREEWAY RAMPS (1, 2 AND 3 LANE)

RD11-TS-5	06-28-19	DESIGN STANDARDS FOR FREEWAYS WITH DEPRESSED MEDIAN (4 AND 6 LANE)

RD11-TS-5A	DESIGN STANDARDS FOR FREEWAYS WITH INDEPENDENT ROADWAYS (4 AND 6 LANE)

RD11-TS-5B	DESIGN STANDARDS FOR FREEWAYS WITH MEDIAN BARRIER (4 AND 6 LANE)

RD11-TS-5W	06-15-21	TYPICAL DETAIL FOR INSIDE LANE WIDENING OF FREEWAYS

RD11-TS-6	TYPICAL CURB & GUTTER SECTIONS WITH SHOULDERS AND WITH GRASS STRIPS

RD11-TS-6A	TYPICAL CURB & GUTTER SECTIONS WITHOUT SHOULDERS AND WITH GRASS STRIPS

RD11-TS-6B	TYPICAL CURB AND GUTTER SECTIONS WITH SHOULDERS AND WITHOUT GRASS STRIPS

RD11-TS-6C	TYPICAL CURB AND GUTTER SECTIONS WITHOUT SHOULDERS AND WITHOUT GRASS STRIPS

RD11-TS-7	07-17-20	DESIGN STANDARDS 2-LANE CURB & GUTTER WITH CONTINUOUS 2-WAY LEFT-TURN LANE WITHOUT GRASS STRIPS

RD11-TS-7A	07-17-20	DESIGN STANDARDS 2-LANE CURB & GUTTER WITH CONTINUOUS 2-WAY LEFT-TURN LANE WITH GRASS STRIPS

RD11-TS-7B	07-17-20	DESIGN STANDARDS 2-LANE HIGHWAYS WITH CONTINUOUS 2-WAY LEFT-TURN LANE

10-101.03	RD11 SLOPE DEVELOPMENT AND RUNOFF LENGTHS

RD11-LR-1	MINIMUM RUNOFF LENGTHS (LR) FOR URBAN HIGHWAYS

RD11-LR-2	MINIMUM RUNOFF LENGTHS (LR) FOR RURAL HIGHWAYS

RD11-S-11	DESIGN AND CONSTRUCTION DETAILS FOR ROADSIDE SLOPE DEVELOPMENT

RD11-S-11A	ROADSIDE DITCH DETAILS FOR DESIGN AND CONSTRUCTION

RD11-S-11B	DESIGN AND CONSTRUCTION DETAILS FOR ROCK CUT SLOPE AND CATCHMENT

10-101.04	RD11 INTERSECTION SIGHT DISTANCE

RD11-SD-1	INTERSECTION SIGHT DISTANCE DESIGN AND GENERAL NOTES

RD11-SD-2	INTERSECTION SIGHT DISTANCE LANDSCAPE AND OBSTRUCTION

RD11-SD-3	INTERSECTION SIGHT DISTANCE 2-LANE ROADWAYS

RD11-SD-4	INTERSECTION SIGHT DISTANCE 4-LANE AND 5-LANE UNDIVIDED ROADWAYS

RD11-SD-5	INTERSECTION SIGHT DISTANCE 4-LANE DIVIDED HIGHWAYS

RD11-SD-6	INTERSECTION SIGHT DISTANCE 6-LANE DIVIDED HIGHWAYS

RD11-SD-7	INTERSECTION SIGHT DISTANCE FOR PASSIVE RAILROAD HIGHWAY GRADE CROSSINGS

10-101.05	RD01 TYPICAL SECTIONS AND DESIGN CRITERIA

RD11 DRAWINGS AVAILABLE

10-101.06	RD01 SLOPE DEVELOPMENT

RD01-S-11	04-04-03	DESIGN AND CONSTRUCTION DETAILS FOR ROADSIDE SLOPE DEVELOPMENT

RD01-S-11A	10-15-02	ROADSIDE DITCH DETAILS FOR DESIGN AND CONSTRUCTION

RD01-S-11B	10-15-02	DESIGN AND CONSTRUCTION DETAILS FOR ROCK CUT SLOPE AND CATCHMENT

RD01-SA-1	10-15-02	SAFETY APPROACH TO UNDERPASSES GRADING DESIGN AND SLOPE PROTECTION

10-101.07	RD01 INTERSECTION SIGHT DISTANCE

RD01-SD-1	INTERSECTION SIGHT DISTANCE DESIGN AND GENERAL NOTES

RD01-SD-2	INTERSECTION SIGHT DISTANCE LANDSCAPE AND OBSTRUCTION

RD01-SD-3	INTERSECTION SIGHT DISTANCE 2-LANE ROADWAYS

RD01-SD-4	INTERSECTION SIGHT DISTANCE 5-LANE AND 4-LANE UNDIVIDED ROADWAYS

RD01-SD-5	INTERSECTION SIGHT DISTANCE 4-LANE DIVIDED HIGHWAYS

RD01-SD-6	INTERSECTION SIGHT DISTANCE 6-LANE DIVIDED HIGHWAYS

RD01-SD-7	INTERSECTION SIGHT DISTANCE FOR PASSIVE RAILROAD HIGHWAY GRADE CROSSINGS

10-101.08	UNDERDRAINS

RD-UD-3	06-28-19	UNDERDRAIN DETAILS

RD-UD-4	06-28-19	UNDERDRAIN LATERAL DETAILS

RD-UD-6	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 1:1 & 2:1 SLOPES

RD-UD-7	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 3:1 & 4:1 SLOPES

RD-UD-8	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 5:1 SLOPES

RD-UD-9	06-28-19	LATERAL UNDERDRAIN ENDWALL DETAIL FOR 6:1 SLOPES

10-102.00 PIPE CULVERTS AND ENDWALLS

10-102.01	PIPE CULVERTS AND FLUME

D-FLU-1	06-28-19	FLUME DETAILS

D-FLU-2	BRIDGE END DRAIN FLUME DETAILS

D-FLU-2A	BRIDGE END DRAIN FLUME DETAILS

D-PB-1	03-01-23	STANDARD DETAILS FOR CONCRETE PIPE INSTALLATION

D-PB-2	03-01-23	STANDARD DETAILS FOR FLEXIBLE PIPE INSTALLATION

D-PB-3	11-30-20	INDUCED TRENCH SOIL EMBANKMENT FOR PIPE CULVERT INSTALLATION

D-PB-4	PIPE COLLAR DETAILS

D-PG-3	06-28-19	FERROUS AND ALUMINUM CORRUGATED METAL PIPE

D-PG-4	06-28-19	FERROUS AND ALUMINUM CORRUGATED METAL PIPE ARCHES

D-PO-1	06-28-19	STANDARD OVAL AND REINFORCED CONCRETE ARCH PIPE CULVERT

D-PS-1	06-28-19	STRUTTING DETAILS FOR CORR. METAL & STRUCTURAL PLATE ROUND PIPE

10-102.02	SAFETY CROSS DRAIN ENDWALLS

D-PE-15A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 15" PIPE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-15B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 15" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-18A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 18" PIPE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-18B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 18" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-24A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 24" PIPE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-24B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 24" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-30A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 30" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-30B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 30" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-36A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 36" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-36B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 36" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-42A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 42" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-42B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 42" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-48A	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 48" PIPE WITH STEEL PIPE GRATE (FOR 3:1, 4:1 & 6:1 SLOPES)

D-PE-48B	06-28-19	TYPE "U" CROSS DRAIN ENDWALL FOR 48" PIPE, BILL OF STEEL AND PRECAST NOTES

D-PE-99	03-04-21	TYPE "U" CROSS DRAIN ENDWALL DETAILS, PIPE GRATE & SKEWED CONNECTION

10-102.03	SAFETY SIDE DRAIN ENDWALLS

D-SEW-1A	07-07-23	TYPE "SAFETY" SIDE ENDWALL WITH STEEL PIPE GRATE, FOR 15" THRU 48" PIPES, 6:1 SLOPE

D-SEW-12D	07-07-23	TYPE “SAFETY” SIDE DRAIN ENDWALL WITH STEEL PIPE GRATE, FOR 18” PIPE, 12:1 SLOPE

SD-MSE-1	06-28-19	SIDE DRAIN MITERED END SECTION

10-102.04	PROTECTED ENDWALLS*

NOTE: THE PROTECTED ENDWALLS MAY NOT BE USED INSIDE THE CLEAR ZONE UNLESS SHIELDED BY GUARDRAIL OR OTHER SAFETY DEVICE.

D-PE-4	06-28-19	STRAIGHT CONCRETE ENDWALLS (PIPE SIZES 18" TO 30")

D-PE-5	06-28-19	STRAIGHT CONCRETE ENDWALLS FOR HORIZONTAL OVAL CONCRETE PIPES (ALL SIZES AND SKEWS)

D-PEW-1	PROTECTED ENDWALLS FOR ROUND & OVAL PIPES (PIPE SIZES 18” TO 72”, ALL SKEWS, 2:1 & 3:1 SLOPES)

D-PEW-2	PROTECTED ENDWALLS FOR ROUND PIPES DETAILS & QUANTITIES (PIPE SIZES 18” TO 72”, ALL SKEWS, 2:1 & 3:1 SLOPES)

D-PEW-3	PROTECTED ENDWALLS FOR OVAL PIPES DETAILS & QUANTITIES (EQU. PIPE SIZES 18” TO 72”, ALL SKEWS, 2:1 & 3:1 SLOPES)

D-PEW-4	PROTECTED STRAIGHT ENDWALLS (PIPE SIZES 18” TO 30” & EQU. OVAL PIPES)

D-PEW-5	RIP-RAP END TREATMENT FOR CORRUGATED METAL PIPE, OVAL AND PIPE ARCH CULVERTS WITH BEVELED ENDS (PIPE SIZES 42” & LARGER)

10-103.00 CATCH BASINS AND MANHOLES

10-103.01	CATCH BASINS

D-CB-DI	ALTERNATE CATCH BASIN DROP INLET DETAILS

D-CB-10LPC	02-20-20	LOW PROFILE LOWERED CURB 32" X 26" RECTANGULAR CONCRETE NO. 10LPC CATCH BASIN

D-CB-10RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 10 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-10S	02-20-20	STANDARD RECTANGULAR CONCRETE N0. 10 CATCH BASIN

D-CB-10SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 10 CATCH BASIN

D-CB-12LP	02-20-20	LOW PROFILE 32" X 32" SQUARE CONCRETE NO. 12LP CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12LPA	ALTERNATE REINFORCEMENT FOR PRECAST CONCRETE 32” X 32” NO. 12LP CATCH BASIN

D-CB-12P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO.12 CATCH BASIN

D-CB-12RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 12 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12RB	02-20-20	STANDARD PRECAST 60" AND 72" CIRCULAR NO. 12 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12RC	02-20-20	STANDARD PRECAST 84" THRU 120" CIRCULAR NO. 12 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-12S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 12 CATCH BASIN

D-CB-12SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-12SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-12SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-12SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 12 CATCH BASIN

D-CB-13P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 13 CATCH BASIN

D-CB-13RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 13 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-13RB	02-20-20	STANDARD PRECAST 60" AND 72" CIRCULAR NO. 13 CATCH BASIN FOR USE WITH 6" VERTICAL CURB

D-CB-13RC	02-20-20	STANDARD PRECAST 84" THRU 120" CIRCULAR NO. 13 CATCH BASIN (FOR USE WITH 6" VERTICAL CURB)

D-CB-13S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 13 CATCH BASIN

D-CB-14P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 14 CATCH BASIN

D-CB-14RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 14RB CATCH BASIN

D-CB-14S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 14 CATCH BASIN

D-CB-14SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 14 CATCH BASIN

D-CB-16S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 16 CATCH BASIN

D-CB-17S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 17 CATCH BASIN

D-CB-25LP	02-20-20	LOW PROFILE 32" X 32" SQUARE CONCRETE NO. 25LP CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25RA	01-28-22	STANDARD PRECAST 48" CIRCULAR NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-25SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 25 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-26P	02-20-20	STANDARD PRECAST RECTANGULAR CONCRETE NO. 26 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-26S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 26 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-27S	02-20-20	STANDARD RECTANGULAR CONCRETE NO. 27 CATCH BASIN (FOR USE WITH 6" SLOPING CURB)

D-CB-31R	02-20-20	STANDARD PRECAST CIRCULAR NO. 31 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-31SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 31 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-31SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 31 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-32LP	02-20-20	STANDARD 80” X 32” RECTANGULAR CONCRETE NO. 32 CATCH BASIN (FOR USE UNDER CONCRETE MEDIUM BARRIER WALL)

D-CB-38RB	03-04-21	STANDARD PRECAST CIRCULAR NO. 38 CATCH BASIN

D-CB-38S	03-04-21	STANDARD 32" X 32" SQUARE CONCRETE NO. 38 CATCH BASIN

D-CB-38SB	03-04-21	STANDARD 4' X 4' SQUARE CONCRETE NO. 38 CATCH BASIN

D-CB-38SC	03-04-21	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 38 CATCH BASIN

D-CB-39RB	03-04-21	STANDARD PRECAST CIRCULAR NO. 39 CATCH BASIN

D-CB-39S	03-04-21	STANDARD 4' X 4' SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-39SC	03-04-21	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-39SD	03-04-21	STANDARD 7' X 7' SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-39SE	03-04-21	STANDARD 9' X 9' SQUARE CONCRETE NO. 39 CATCH BASIN

D-CB-40S	03-04-21	STANDARD 4' X 8' RECTANGULAR CONCRETE NO. 40 CATCH BASIN

D-CB-40SE	03-04-21	STANDARD 9’ X 9’ SQUARE CONCRETE NO. 40. CATCH BASIN

D-CB-41LP	02-20-20	LOW PROFILE 32" X 32" SQUARE CONCRETE NO. 41LP CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41P	02-20-20	STANDARD PRECAST 4' x 3' RECTANGULAR CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41S	02-20-20	STANDARD 4' X 3' RECTANGULAR CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-41SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 41 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-42RB	02-20-20	STANDARD PRECAST CIRCULAR NO. 42 CATCH BASIN

D-CB-42S	02-20-20	STANDARD 32" X 32" SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-42SB	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-42SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-42SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 42 CATCH BASIN

D-CB-43R	02-20-20	STANDARD PRECAST CIRCULAR NO. 43R CATCH BASIN

D-CB-43SB	02-20-20	STANDARD 8' X 4' RECTANGULAR CONCRETE NO. 43SB CATCH BASIN

D-CB-43SC	02-20-20	STANDARD 8' X 5' 2" RECTANGULAR CONCRETE NO. 43SC CATCH BASIN

D-CB-44SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 44 CATCH BASIN

D-CB-45S	02-20-20	STANDARD 8' X 4' RECTANGULAR CONCRETE NO. 45 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-46SE	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 46 CATCH BASIN (FOR USE UNDER CONCRETE MEDIAN BARRIER WALL)

D-CB-51SC	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 51 CATCH BASIN (FOR USE IN FRONT OF CONCRETE RETAINING WALL)

D-CB-51SD	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 51 CATCH BASIN (FOR USE IN FRONT OF CONCRETE RETAINING WALL)

D-CB-51SE	02-20-20	STANDARD 9’ X 9’ SQUARE CONCRETE NO. 51 CATCH BASIN

D-CB-52SE	02-20-20	STANDARD 9’ x 9’ SQUARE CONCRETE NO. 52 CATCH BASIN

D-CB-99	02-20-20	MISCELLANEOUS DETAILS FOR RECTANGULAR STRUCTURES

D-CB-99R	01-28-22	MISCELLANEOUS DETAILS FOR ROUND STRUCTURES

D-CB-99RA	10-29-21	BILL OF STEEL FOR ROUND CATCH BASIN LIDS

D-CB-99RB	02-20-20	ROUND JUNCTION BOX SPRING DRAIN BOX

D-CBB-12A	06-28-19	TYPE ‘B’ CAST IRON FRAME, GRATE & VERTICAL INLET DETAILS FOR NOS. 10, 12, 14, 16 & 17 TYPE CATCH BASINS

D-CBB-12B	06-28-19	TYPE ‘B’ CAST IRON FRAME, GRATE & 6" SLOPING INLET DETAILS FOR NOS. 25, 26 & 27 TYPE CATCH BASINS

D-CBB-12D	07-07-23	TYPE "B" CAST IRON FRAME, GRATE & CURB HOOD DETAILS FOR NOS. 12, 14, 16 & 17 TYPE CATCH BASINS

D-CBB-13	06-28-19	TYPE ‘B’ CAST IRON FRAME, GRATE & VERTICAL INLET DETAILS FOR NO. 13 TYPE CATCH BASINS

D-CBB-31	02-20-20	TYPE “B” CAST IRON FRAME, GRATE & INLET DETAILS FOR NOS. 31, 41, 45, 46, & 51 TYPE CATCH BASINS

D-CBB-42	10-29-21	CAST IRON GRATE DETAILS FOR NOS. 42, 43 & 44 TYPE CATCH BASINS

10-103.02	JUNCTION BOXES

D-JBS-1	02-20-20	STANDARD 32" X 32" SQUARE CONCRETE NO. 1 JUNCTION BOX

D-JBS-2	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 2 JUNCTION BOX

D-JBS-3	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 3 JUNCTION BOX

D-JBS-4	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 4 JUNCTION BOX

D-JBS-5	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 5 JUNCTION BOX

10-103.03	MANHOLES

D-MH-2	02-20-20	STANDARD PRECAST NO. 3 MANHOLE

D-MH-3	02-20-20	TYPICAL DESIGN OF LIDS FOR NO. 3 MANHOLE

D-MH-4	02-20-20	STANDARD NO. 3 MANHOLE CASTINGS AND STEPS

D-MH-5	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 3 MANHOLE

D-MH-6	02-20-20	STANDARD 7' X 7' SQUARE CONCRETE NO. 3 MANHOLE

D-MH-7	02-20-20	STANDARD 9' X 9' SQUARE CONCRETE NO. 3 MANHOLE

10-103.04	PRECAST RISERS

D-RF-1	05-04-22	STANDARD PRECAST RISER

10-103.05	SPRING DRAIN BOXES

D-SDS-1	02-20-20	STANDARD 32" X 32" SQUARE CONCRETE NO. 1 SPRING DRAIN BOX

D-SDS-2A	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 2A SPRING DRAIN BOX

D-SDS-2B	02-20-20	STANDARD 4' X 4' SQUARE CONCRETE NO. 2B SPRING DRAIN BOX

D-SDS-3A	02-20-20	STANDARD 5' 2" X 5' 2" SQUARE CONCRETE NO. 3A SPRING DRAIN BOX

10-103.06	SLOTTED AND TRENCH DRAINS

D-SLD-1	02-20-20	SLOTTED DRAINS

D-SLD-2	02-20-20	SLOTTED DRAINS

D-SLD-3	02-20-20	SLOTTED DRAINS

D-TD-1	07-07-23	TRENCH DRAIN

10-104.00 NATURAL STREAM DESIGN

10-104.01	DEFLECTORS, VANES AND ENERGY DISSIPATORS

D-NSD-13	05-01-20	LONGITUDINAL STONE TOE

D-NSD-21	05-01-20	BOULDER CLUSTERS

D-NSD-22	05-01-20	BOULDER CROSS VANE

D-NSD-23	05-01-20	BOULDER CROSS VANE WITH STEP

D-NSD-24	05-01-20	BOULDER W-WEIR

D-NSD-25	05-01-20	BOULDER VANES AND J-HOOK

D-NSD-26	11-30-20	LOG VANES, ROOT WADS, AND BOULDER J-HOOK

D-NSD-27	11-30-20	LOG AND BOULDER STEP POOLS

D-NSD-28	05-01-20	BOULDER RIFFLES

D-NSD-28A	11-30-20	LOG RIFFLES

D-NSD-29	05-01-20	CONSTRUCTED ALLUVIAL RIFFLE

D-NSD-30	05-01-20	SUBSTRATE RESTORATION

D-NSD-31	05-01-20	CLAY CHANNEL PLUG

D-NSD-32	05-01-20	WOOD TOE WITH GEO-LIFTS

D-NSD-32A	05-01-20	BOULDER TOE WITH GEO-LIFTS

D-NSD-33	05-01-20	COIR FIBER EROSION CONTROL BLANKET AND

COIR FIBER ROLLS

D-NSD-34	05-01-20	LIVE STAKES AND LIVE SILTATION

D-NSD-35	05-01-20	LIVE FASCINES

D-NSD-36	05-01-20	BRUSH MATTRESS

D-NSD-37	05-01-20	SPECIAL NOTES FOR NATURAL STREAM DESIGN

10-105.00 ROADWAY, PAVEMENT APPURTENANCES, AND FENCES

10-105.01	CONCRETE PAVEMENT

RP-CS-1	05-01-20	CONCRETE SHOULDER RUMBLE STRIP DETAIL (FOR 4-LANE DIVIDED HIGHWAY)

RP-CS-2	05-01-20	CONCRETE SHOULDER RUMBLE STRIP DETAIL (FOR 6-LANE OR WIDER DIVIDED HIGHWAY)

RP-CS-3	CONCRETE SHOULDER MILLED RUMBLE STRIP DETAILS

RP-J-1	05-01-20	PORTLAND CEMENT CONCRETE PAVEMENT JOINT TYPES AND SPACING

RP-J-3	05-01-20	PORTLAND CEMENT CONCRETE PAVEMENT JOINT TYPES AND SPACING

RP-J-5	05-01-20	TYPICAL ACCELERATION AND DECELERATION LANE JOINT TYPES AND SPACING FOR CONCRETE RAMPS

RP-J-7	05-01-20	CONCRETE RAMP JOINT TYPES AND SPACING

RP-J-9	05-01-20	CONTRACTION AND CONSTRUCTION JOINTS FOR CONCRETE PAVEMENT

RP-J-11	05-01-20	3/4" AND 1 3/4" EXPANSION AND EDGE PAVEMENT JOINTS

RP-J-13	05-01-20	3/4" AND 1 3/4" ELASTOMERIC COMPRESSION JOINT SEALS

RP-J-15	05-01-20	LONGITUDINAL CONTRACTION AND CONSTRUCTION JOINTS

RP-J-17	05-01-20	DOWEL ASSEMBLY DEVICES

RP-J-18	01-28-22	DOWEL ASSEMBLY DEVICES

RP-J-19	05-01-20	DOWEL ASSEMBLY DEVICES

RP-J-23	01-28-22	CONCRETE PAVEMENT REPAIR DETAILS

RP-J-24	05-01-20	CONCRETE PAVEMENT SPALL AND RANDOM CRACK REPAIR DETAILS

RP-J-25	05-01-20	CONCRETE PAVEMENT JOINT REPAIR DETAILS

RP-J-26	STANDARD CONSTRUCTION DETAILS FOR ROUNDABOUTS

10-105.02	INTERSECTIONS

RP-D-15	06-15-21	DETAILS OF STANDARD CONCRETE DRIVEWAYS

RP-D-16	10-29-21	DETAILS OF LOWERED STANDARD CONCRETE DRIVEWAYS

RP-DHO-1	05-01-20	MEDIAN OPENINGS ON 4-LANE DIVIDED HIGHWAY

RP-DHO-2	07-07-23	MEDIAN OPENING DETAILS FOR RESTRICTED CROSSING & J-TURN INTERSECTIONS

RP-I-5	05-01-20	EXAMPLES OF STREET & ALLEY INTERSECTIONS

RP-PMR-1	05-01-20	STANDARD DETAILS FOR PROPOSED PERMANENT MAINTENANCE RAMP

RP-R-1	10-16-20	STANDARD RAMP DETAILS FOR ROADWAYS AND DRIVEWAYS

10-105.03	CURBS

RP-SC-1	05-04-22	SLOPING CONCRETE CURB AND CURB AND GUTTER

RP-VC-10	03-04-21	VERTICAL CONCRETE CURB AND CURB AND GUTTER (FOR 8” TO 12” GUTTER DEPTH)

RP-VC-11	03-04-21	VERTICAL CONCRETE CURB AND CURB AND GUTTER (FOR 6” & 7” GUTTER DEPTH)

10-105.04	WALLS

W-CIP-1	05-01-20	ROADWAY FEATURES AT CAST IN PLACE RETAINING WALL

W-MSE-1	05-01-20	ROADWAY FEATURES FOR MSE SEGMENTAL PRECAST FACING RETAINING WALL

W-MSE-2	05-01-20	ROADWAY FEATURES FOR MSE MODULAR BLOCK FACING RETAINING WALL

W-SG-1	05-01-20	STANDARD GRAVITY-TYPE RETAINING WALLS

W-SP-1	05-01-20	ROADWAY FEATURES AT SOLDIER PILE AND SOIL ANCHORED RETAINING WALLS

10-105.05	FENCES AND RIGHT-OF-WAY MARKERS

S-F-1	03-01-23	HIGH VISIBILITY FENCE

S-F-10	07-17-20	STANDARD RIGHT-OF-WAY STOCK FENCE

S-F-10A	06-28-19	STANDARD RIGHT-OF-WAY STOCK FENCE WITH TIMBER POSTS

S-F-10B	06-28-19	STANDARD RIGHT-OF-WAY CHAIN LINK FENCE

S-F-10C	06-28-19	RIGHT-OF-WAY FENCE AT BRIDGES AND BOX CULVERTS

S-F-10D	06-28-19	RIGHT-OF-WAY FENCE LOCATIONS AT INTERCHANGES

S-FG-11	06-28-19	STANDARD STOCK FENCE GATE

S-FG-20	06-28-19	EXAMPLES OF WATER GATES AND WATER CROSSINGS

S-RP-2	06-28-19	STANDARD CONCRETE RIGHT-OF-WAY MARKERS

10-106.00 MULTIMODAL

10-106.01	CURB RAMPS

MM-CR-1	06-28-19	DETECTABLE WARNING SURFACE PLACEMENT ON CURB RAMPS

MM-CR-2	PERPENDICULAR CURB RAMP

MM-CR-3	PARALLEL CURB RAMP

MM-CR-4	PEDESTRIAN REFUGE

MM-CR-5	06-28-19	SINGLE CROSSING CURB RAMP IN CURVE

MM-CR-6	DUAL CROSSING CURB RAMP PLACED OUTSIDE CURVE

MM-CR-7	CURB RAMPS IN CURVE Bl-DIRECTIONAL DUAL CROSSING

MM-CR-8	MONO-DIRECTIONAL SINGLE CROSSWALK CURB RAMP DETAILS

MM-CR-9	ALTERNATIVE CURB RAMP DETAILS

10-106.02	PAVEMENT MARKING

MM-PM-1	SIGNING AND PAVEMENT MARKINGS AT INTERSECTION CROSSINGS FOR SHARED-USE PATHS

MM-PM-2	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANE OR ROUTES

MM-PM-3	06-15-21	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANES ON URBAN ROADWAYS

MM-PM-4	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANES

MM-PM-5	05-04-22	SIGNING AND PAVEMENT MARKINGS FOR BICYCLE LANES AT INTERSECTIONS

10-106.03	SAFETY RAIL

MM-BPR-1	01-28-22	BIKE AND PEDESTRIAN SAFETY RAIL

MM-BPR-2	10-16-20	BIKE AND PEDESTRIAN MEDIAN BARRIER RAIL

MM-BPR-3	BARRIER SLOPED END TREATMENT

MM-VPR-1	VEHICLE AND PEDESTRIAN SAFETY RAIL

10-106.04	SIDEWALK

MM-PS-1	DETAILS FOR PEDESTRIAN STEPS AND HANDRAILS

MM-SW-1	07-07-23	DETAILS FOR CONCRETE SIDEWALKS

MM-SW-2	ALTERNATE DETAILS FOR CONCRETE SIDEWALK (REHABILITATION)

10-106.05	TYPICAL SECTION

MM-TS-1	06-15-21	BIKE ACCOMMODATION DESIGN GUIDANCE

MM-TS-2	06-15-21	LATERAL OFFSETS FOR SIDEWALK AND SHARED USE PATH

MM-TS-3	01-28-22	SEPARATED SHARED USE PATH TYPICAL SECTIONS

10-107.00 SAFETY DESIGN AND GUARDRAILS

10-107.01	CLEAR ZONE AND SAFETY PLANS

S-CZ-1	06-28-19	CLEAR ZONE CRITERIA

S-PL-1	03-01-23	SAFETY PLAN FOR BARRIER LENGTH OF NEED

S-PL-1A	03-01-23	SAFETY PLAN FOR BARRIER LENGTH OF NEED (FOR RIGID OBJECTS)

S-PL-1B	03-01-23	SAFETY PLAN FOR BARRIER LENGTH OF NEED ON CURVED ROADWAYS

S-PL-3	03-01-23	SAFETY PLAN MINIMUM INSTALLATION AT BRIDGE ENDS

S-PL-4	06-28-19	SAFETY PLAN FOR BRIDGE PIERS IN CLEAR ZONE

S-PL-4A	SAFETY PLAN FOR BRIDGE PIERS IN CLEAR ZONE & OUT OF CLEAR ZONE

S-PL-5	06-28-19	SAFETY PLAN FOR BRIDGE ENDS IN MEDIANS

S-PL-6	06-15-21	SAFETY PLAN SAFETY HARDWARE PLACEMENT ON OUTSIDE EDGE

S-PL-6A	06-28-19	SAFETY PLAN SAFETY HARDWARE PLACEMENT IN MEDIAN

10-107.02	CABLE BARRIER

S-CB-1	07-07-23	CABLE BARRIER PLACEMENT

S-CB-2	07-07-23	HIGH TENSION CABLE BARRIER

10-107.03	CRASH CUSHIONS

S-CC-1	03-01-23	CRASH CUSHION

S-CC-2	06-28-19	CRASH CUSHION (GATING) BARREL ARRAY

10-107.04	GUARDRAIL DETAILS

S-GR31-1	06-15-21	GUARDRAIL DETAILS

S-GR31-1A	06-28-19	GUARDRAIL AND BLOCK-OUT DETAILS

S-GR31-1B	GUARDRAIL FASTENING HARDWARE

S-GR31-1C	07-07-23	GUARDRAIL GENERAL NOTES AND POST DETAILS

S-GR31-1D	03-01-23	GUARDRAIL POST PLACEMENT IN ROCK

10-107.05	GUARDRAIL CONNECTIONS

S-GRC-4	07-07-23	GUARDRAIL CONNECTION TO BRIDGE RAILING CONCRETE PARAPET

S-GRC-5	02-28-20	GUARDRAIL CONNECTION TO BRIDGE ENDS (TRAILING ENDS)

S-GRC-6	07-07-23	GUARDRAIL CONNECTION TO BRIDGE ENDS FOR LOW SPEED ROADWAYS

10-107.06	GUARDRAIL (SPECIAL CASES)

S-CPW-1	CURVED PARAPET WALL ≤ 40 M.P.H.

S-GRS-1	06-15-21	SPECIAL CASE LONG SPAN GUARDRAIL 1 POST, 2 OR 3 POSTS OMITTED

S-GRS-2	01-28-22	SPECIAL CASE GUARDRAIL ATTACHMENT TO CONCRETE DECKS

S-GRS-3	06-28-19	SPECIAL CASE GUARDRAIL FOOTING

S-GRS-4	05-04-22	SPECIAL CASE GUARDRAIL HEIGHT TRANSITION DETAIL

S-GRS-5	SPECIAL CASE WEAK-POST GUARDRAIL ATTACHMENT TO CULVERT

S-GRS-5A	06-15-21	WEAK-POST GUARDRAIL ASSEMBLY DETAILS FOR TYPE 1 & 2

S-GRS-5B	WEAK-POST GUARDRAIL ASSEMBLY DETAILS FOR TYPE 3 & 4

S-GRS-6	SPECIAL CASE FLEXIBITLTY ON GUARDRAIL POST INSTALLATIONS

S-GRS-7	SHORT – RADIUS GUARDRAIL SYSTEM (SRGS)

S-GRS-7A	SHORT – RADIUS GUARDRAIL SYSTEM (SRGS) DETAILS

10-107.07	GUARDRAIL TERMINALS

S-GRT-1	10-29-21	TYPE 12 GUARDRAIL TERMINAL BURIED-IN-BACKSLOPE

S-GRT-1A	LAYOUT OF FLARED GUARDRAIL (TL- 3)

S-GRT-1B	LAYOUT OF FLARED GUARDRAIL (TL- 2)

S-GRT-2	06-28-19	TYPE 38 GUARDRAIL END TERMINAL

S-GRT-2P	10-16-20	EARTH PAD FOR TYPE 38 AND TYPE 21 TERMINAL

S-GRT-2R	06-28-19	EARTH PAD FOR TYPE 38 AND TYPE 21 TERMINAL (RETROFIT)

S-GRT-3	06-28-19	TYPE 21 GUARDRAIL END TERMINAL

10-107.08	GUARDRAIL ANCHORS

S-GRA-1	06-28-19	TYPE 12 GUARDRAIL ANCHOR

S-GRA-1A	06-28-19	GUARDRAIL ANCHOR FOR TYPE 12 TERMINAL (ALTERNATIVE)

S-GRA-3	06-15-21	TYPE 13 GUARDRAIL ANCHOR

S-GRA-4	03-01-23	IN-LINE GUARDRAIL ANCHOR TO PRIVATE DRIVE

S-GRA-5	06-28-19	FLARED GUARDRAIL ANCHOR

10-107.09	CONCRETE MEDIAN BARRIERS

S-SSMB-1	01-28-22	32” SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-1A	10-29-21	36” SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-2	10-29-21	51” SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-3	10-29-21	51” HALF SIZE SINGLE SLOPE CONCRETE BARRIER WALL

S-SSMB-4	07-17-20	FLARED SINGLE SLOPE CONCRETE MEDIAN BARRIER WALL (VERTICAL BACK)

S-SSMB-5	05-01-20	SINGLE SLOPE MEDIAN BARRIER WALL CATCH BASIN DETAIL

S-SSMB-6	06-28-19	32"CONCRETE SINGLE SLOPE BARRIER WALL WITH SINGLE GUARDRAIL ATTACHMENT

S-SSMB-6A	36” CONCRETE SINGLE SLOPE BARRIER WALL FOR ATTACHING GUARDRAIL

S-SSMB-6B	DUAL GUARDRAIL ATTACHMENT TO SINGLE SLOPE 36” BARRIER WALL

S-SSMB-6C	SINGLE GUARDRAIL ATTACHMENT TO SINGLE SLOPE 36” BARRIER WALL

S-SSMB-6D	51” CONCRETE SINGLE SLOPE BARRIER WALL FOR ATTACHING GUARDRAIL

S-SSMB-6E	DUAL GUARDRAIL ATTACHMENT TO SINGLE SLOPE 51” BARRIER WALL

S-SSMB-6F	SINGLE GUARDRAIL ATTACHMENT TO SINGLE SLOPE 51” BARRIER WALL

S-SSMB-7	05-01-20	FOOTING DETAILS FOR OVERHEAD SIGN STRUCTURE 32” MEDIAN BARRIER WALL

S-SSMB-8	05-01-20	FOOTING DETAILS FOR OVERHEAD SIGN STRUCTURE 51” MEDIAN BARRIER WALL

S-SSMB-9	10-29-21	SINGLE SLOPE BARRIER WALL FOR GRADE SEPARATED MEDIAN

S-SSMB-10	SPECIAL DETAIL FOR CONCRETE MEDIAN BARRIER WALL BARRIER WALL TRANSITION FROM 32” TO 51”

10-107.10	GUARDRAIL MAINTENANCE

S-GR28-1M	06-15-21	W-BEAM & THRIE BEAM BARRIER RAIL AND RUB RAIL DETAILS

S-GR28-2M	06-28-19	GUARDRAIL HARDWARE DETAILS

S-GR28-3M	01-28-22	GUARDRAIL HEIGHT ADJUSTMENT

S-GR28-4M	06-28-19	GUARDRAIL TERMINAL ANCHOR TYPE 13

S-GR28-5M	06-28-19	MEDIAN DIVIDER GUARDRAIL

S-GR28-6M	10-29-21	GUARDRAIL ATTACHMENT TO CONCRETE DECKS

S-GR28-7M	06-28-19	GUARDRAIL ATTACHMENT TO BRIDGE END DETAILS MAINTENANCE ONLY

S-GRC-1M	GUARDRAIL CONNECTION TO BRIDGE ENDS OR BARRIER WALL

S-GRC-2M	GUARDRAIL CONNECTION TO BRIDGE END FOR LOCAL ROADS (ADT<2000)

S-GRC-3M	MEDIAN DIVIDER GUARDRAIL TRANSITION TO CONCRETE MEDIAN BARRIER

S-PL-2M	SAFETY PLAN AT SIDE ROADS OR PRIVATE DRIVES

S-SSMB-6M	GUARDRAIL ATTACHMENT TO EXISTING SINGLE SLOPE CONCRETE BARRIER WALL

10-108.00 DESIGN - TRAFFIC CONTROL

10-108.01	PAVEMENT MARKINGS

T-M-1	06-28-19	DETAILS OF PAVEMENT MARKINGS FOR CONVENTIONAL ROADS AND MARKING ABBREVIATIONS

T-M-2	06-28-19	DETAILS OF PAVEMENT MARKINGS FOR CONVENTIONAL ROADS

T-M-3	07-07-23	MARKING STANDARDS FOR TRAFFIC ISLANDS, PAVED SHOULDERS AND MEDIANS FOR CONVENTIONAL ROADS

T-M-4	07-17-20	STANDARD INTERSECTION PAVEMENT MARKINGS

T-M-4A	03-01-23	STANDARD UNSIGNALIZED MID-BLOCK CROSSING

T-M-4B	03-01-23	STANDARD SIGNALIZED MID-BLOCK CROSSING

T-M-4C	PEDESTRIAN GATEWAY TREATMENT

T-M-5	03-01-23	MARKING DETAIL FOR FREEWAYS

T-M-6	03-01-23	MARKING DETAIL FOR EXPRESSWAY AND FREEWAY INTERCHANGES

T-M-7	06-28-19	GORE MARKING DETAILS FOR EXPRESSWAY & FREEWAY INTERCHANGES

T-M-8	06-28-19	MARKING DETAILS FOR EXPRESSWAYS & FREEWAYS

T-M-9	05-01-23	PAVEMENT MARKING AND SIGNING DETAILS FOR RAMP INTERSECTIONS

T-M-9A	PAVEMENT MARKING AND SIGNING DETAILS FOR RAMP INTERSECTIONS

T-M-9B	PAVEMENT MARKING AND SIGNING DETAILS FOR RAMP INTERSECTIONS

T-M-15	06-28-19	ASPHALT SHOULDER RUMBLE STRIP INSTALLATION DETAILS FOR INTERSTATE AND ACCESS CONTROLLED ROUTES

T-M-15A	06-28-19	ASPHALT SHOULDER RUMBLE STRIP INSTALLATION DETAILS FOR NON-ACCESS CONTROLLED RURAL ROUTES

T-M-16	03-04-21	RUMBLE STRIPE INSTALLATION LAYOUT

T-M-16A	02-03-20	RUMBLE STRIPE DETAILS FOR EDGE OF PAVEMENT AND CENTERLINE

T-M-17	05-04-22	PAVEMENT MARKING DETAILS FOR ROUNDABOUTS

T-M-18	10-29-21	FLEXIBLE DELINEATOR DETAILS

T-M-18A	DELINEATOR MOUNTING DETAILS

T-M-19	07-07-23	PAVEMENT MARKING DETAILS FOR RESTRICTED CROSSING & J-TURN INTERSECTION.

10-108.02	WORK ZONES

T-WZ-10	04-02-12	ADVANCE ROAD WORK SIGNING ON HIGHWAYS AND FREEWAYS

T-WZ-11	03-04-21	ONE LANE CLOSURE DETAIL ON DIVIDED HIGHWAYS

T-WZ-12	03-04-21	ONE LANE CLOSURE DETAIL FOR BRIDGES ON DIVIDED HIGHWAYS

T-WZ-13	05-01-20	TWO-OUTSIDE LANE CLOSURE FOR EXPRESSWAY AND FREEWAYS

T-WZ-14	03-04-21	TWO-OUTSIDE LANE CLOSURE FOR INTERSTATES AND EXPRESSWAYS

T-WZ-15	05-01-20	INTERIOR LANE CLOSURE FOR FREEWAYS

T-WZ-16	03-04-21	LANE SHIFT FOR DIVIDED HIGHWAYS AND FREEWAYS

T-WZ-18	07-07-23	SHOULDER CLOSURE DETAIL FOR FREEWAYS AND DIVIDED HIGHWAYS

T-WZ-19	03-04-21	MEDIAN CROSS-OVER DETAIL ON FREEWAYS

T-WZ-20	12-18-99	GEOMETRIC MEDIAN CROSS-OVER DETAIL ON DIVIDED HIGHWAYS

T-WZ-21	05-01-20	LANE CLOSURE WITH LEFT HAND MERGE AND LANE SHIFT

T-WZ-30	09-01-05	TRAFFIC CONTROL 2-LANE, 2-WAY DIVERSION (40 MPH OR LESS)

T-WZ-31	09-01-05	TRAFFIC CONTROL 2-LANE, 2-WAY DIVERSION (GREATER THAN 40 MPH)

T-WZ-32	11-30-20	TRAFFIC CONTROL PLAN SIGNAL LAYOUT FOR TRAFFIC SIGNAL AT TWO LANE BRIDGE RECONSTRUCTION SITE

T-WZ-33	05-27-98	TRAFFIC CONTROL PLAN FOR CLOSE INTERSECTION CONDITIONS USING TRAFFIC SIGNAL AT TWO LANE BRIDGE RECONSTRUCTION SITE

T-WZ-34	09-01-05	TRAFFIC CONTROL PLAN GENERAL NOTES FOR TRAFFIC SIGNAL AT TWO LANE BRIDGE RECONSTRUCTION SITE

T-WZ-35	04-02-12	TRAFFIC CONTROL PLAN PAY ITEM AND SIGN DETAILS FOR TRAFFIC SIGNAL AT TWO LANE BRIDGE RECONSTRUCTION SITE

T-WZ-36	03-05-17	LANE CLOSURE ON LOW-VOLUME 2-LANE HIGHWAY

T-WZ-40	03-05-17	RIGHT LANE CLOSURES AT NEAR SIDE OF INTERSECTIONS

T-WZ-41	03-05-17	LEFT LANE CLOSURES AT NEAR SIDE OF INTERSECTIONS

T-WZ-42	03-05-17	CENTER LANE CLOSURES AT NEAR SIDE OF INTERSECTIONS

T-WZ-50	04-02-12	TRAFFIC CONTROL FOR SIGNALS ONLY PROJECTS ON 2 OR 3 LANE MAJOR ROUTES

T-WZ-51	04-02-12	TRAFFIC CONTROL FOR SIGNALS ONLY PROJECTS ON 4 OR 5 LANE MAJOR ROUTES

T-WZ-52	04-02-12	TRAFFIC CONTROL FOR SIGNALS ONLY PROJECTS ON 4 OR 5 LANE MAJOR AND MINOR ROUTES

T-WZ-53	04-02-12	TRAFFIC CONTROL FOR SIGNALS ONLY PROJECTS ON 4 OR MORE LANE DIVIDED MAJOR ROUTES

T-WZ-54	04-02-12	TRAFFIC CONTROL FOR SIGNALS ONLY PROJECTS ON 4 OR MORE LANE DIVIDED MAJOR ROUTES AND 4 OR MORE LANE MINOR ROUTES

T-WZ-55	10-29-21	SIDEWALK TRAFFIC CONTROL

T-WZ-56	05-15-22	TRANSVERSE RUMBLE STRIP USE WITHIN WORK ZONES

T-WZ-60	FREEWAY RESURFACING SIGNING LAYOUT

T-WZ-61	05-15-22	ROLLING ROADBLOCK DETAIL FOR DIVIDED HIGHWAYS

T-WZ-62	CONSTRUCTION ACCESS/EMERGENCY PULL-OFF ON FREEWAYS

T-WZ-63	WORK ZONE IN THE VICINITY OF AN ENTRANCE RAMP

T-WZ-64	WORK ZONE IN THE VICINITY OF AN EXIT

T-WZ-FAB1	FLASHING YELLOW ARROW BOARD

T-WZ-PBR1	12-09-22	INTERCONNECTED PORTABLE BARRIER RAIL

T-WZ-PBR2	02-28-20	DETAILS FOR WORK ZONE CHANNELIZATION DEVICES

T-WZ-PCB1	12-09-22	10 FOOT PORTABLE CONCRETE BARRIER RAIL

T-WZ-PCB2	12-09--22	20 FOOT PORTABLE CONCRETE BARRIER RAIL

T-WZ-PCB2A	12-09-22	20 FOOT PORTABLE CONCRETE BARRIER RAIL STIFFENER TUBE

T-WZ-PCB3	01-28-22	PORTABLE CONCRETE BARRIER RAIL DETAILS

T-WZ-PCB4	12-09-22	PORTABLE CONCRETE BARRIER RAIL ANCHOR PIN DETAILS

10-109.00 EROSION PREVENTION AND SEDIMENT CONTROL

10-109.01	DEWATERING DEVICES

EC-STR-1	08-01-12	DEWATERING STRUCTURE

EC-STR-2	08-01-12	SEDIMENT FILTER BAG

10-109.02	SLOPE DEVICES

EC-STR-3B	06-15-21	SILT FENCE

EC-STR-3C	03-01-23	SILT FENCE WITH WIRE BACKING

EC-STR-3D	03-01-23	ENHANCED SILT FENCE

EC-STR-3E	04-01-08	SILT FENCE FABRIC JOINING DETAILS

EC-STR-8	06-10-14	FILTER SOCK

EC-STR-27	08-01-12	TEMPORARY SLOPE DRAIN AND BERM

EC-STR-29	08-01-12	PERMANENT SLOPE DRAIN PIPE

EC-STR-34	05-04-22	EROSION CONTROL BLANKET FOR SLOPE INSTALLATION

EC-STR-35	08-01-12	FILTER BERMS

EC-STR-37	06-10-14	SEDIMENT TUBE

10-109.03	DITCH DEVICES

EC-STR-4	08-01-12	ENHANCED SILT FENCE CHECK (TRAPEZOIDAL DITCH)

EC-STR-4A	08-01-12	ENHANCED SILT FENCE CHECK (V-DITCH)

EC-STR-4B	08-01-12	ENHANCED SILT FENCE CHECK DETAILS

EC-STR-6	11-30-20	ROCK CHECK DAM

EC-STR-6A	05-06-16	ENHANCED ROCK CHECK DAM

EC-STR-7	05-04-22	SEDIMENT TRAP WITH CHECK DAM

EC-STR-55	08-01-12	GABION CHECK DAM

EC-STR-56	04-01-08	GABION CHECK DAM DESIGN TABLES

EC-STR-57	04-01-08	GABION ASSEMBLY DETAILS

EC-STR-58	04-01-08	GABION ASSEMBLY DETAILS

EC-STR-59	08-01-12	GABION CHECK DAM GENERAL NOTES AND COMPONENT PROPERTIES

EC-STR-61	03-16-17	LEVEL SPREADERS

10-109.04	INLET PROTECTION

EC-STR-11	03-16-17	CULVERT PROTECTION TYPE 1

EC-STR-19	04-01-08	CATCH BASIN PROTECTION

EC-STR-39	08-01-12	CURB INLET PROTECTION TYPE 1 & 2

EC-STR-39A	08-01-12	CURB INLET PROTECTION TYPE 3 & 4

EC-STR-40	CATCH BASIN FILTER ASSEMBLY FOR CIRCULAR STRUCTURES

EC-STR-41	CATCH BASIN FILTER ASSEMBLY (TYPE 1)

EC-STR-41A	CATCH BASIN FILTER ASSEMBLY (TYPE 1) SLIPCOVER DETAILS

EC-STR-42	CATCH BASIN FILTER ASSEMBLY (TYPE 2)

EC-STR-42A	CATCH BASIN FILTER ASSEMBLY (TYPE 2) SLIPCOVER DETAILS

EC-STR-43	CATCH BASIN FILTER ASSEMBLY (TYPE 3)

EC-STR-43A	CATCH BASIN FILTER ASSEMBLY (TYPE 3) SLIPCOVER DETAILS

EC-STR-44	CATCH BASIN FILTER ASSEMBLY (TYPE 4)

EC-STR-44A	CATCH BASIN FILTER ASSEMBLY (TYPE 4) SLIPCOVER DETAILS

EC-STR-45	CATCH BASIN FILTER ASSEMBLY (TYPE 5)

EC-STR-45A	CATCH BASIN FILTER ASSEMBLY (TYPE 5) SLIPCOVER DETAILS

EC-STR-46	CATCH BASIN FILTER ASSEMBLY (TYPE 6)

EC-STR-46A	CATCH BASIN FILTER ASSEMBLY (TYPE 6) SLIPCOVER DETAILS

EC-STR-47	CATCH BASIN FILTER ASSEMBLY (TYPE 7)

EC-STR-47A	CATCH BASIN FILTER ASSEMBLY (TYPE 7) SLIPCOVER DETAILS

EC-STR-48	CATCH BASIN FILTER ASSEMBLY (TYPE 8)

EC-STR-48A	CATCH BASIN FILTER ASSEMBLY (TYPE 8) SLIPCOVER DETAILS

EC-STR-49	CATCH BASIN FILTER ASSEMBLY (TYPE 9)

EC-STR-49A	CATCH BASIN FILTER ASSEMBLY (TYPE 9) SLIPCOVER DETAILS

EC-STR-50	CATCH BASIN FILTER ASSEMBLY (TYPE 10)

EC-STR-50A	CATCH BASIN FILTER ASSEMBLY (TYPE 10) SLIPCOVER DETAILS

EC-STR-51	CATCH BASIN FILTER ASSEMBLY (TYPE 11)

EC-STR-51A	CATCH BASIN FILTER ASSEMBLY (TYPE 11) SLIPCOVER DETAILS

10-109.05	DETAINING DEVICES

EC-STR-12	08-01-12	ROCK SEDIMENT DAM

EC-STR-13	08-01-12	ROCK AND EARTH SEDIMENT EMBANKMENT

EC-STR-15	08-01-12	SEDIMENT BASIN

EC-STR-16	08-01-12	SEDIMENT BASIN RISER AND COLLAR APPURTENANCES

EC-STR-17	08-01-12	SEDIMENT BASIN EMBANKMENT DETAILS

EC-STR-18	SEDIMENT BASIN FLOATING OUTLET STRUCTURE

EC-STR-21	05-04-22	PERMANENT RIPRAP BASIN ENERGY DISSIPATORS

10-109.06	IN-STREAM DEVICES

EC-STR-11A	08-01-12	CULVERT PROTECTION TYPE 2

EC-STR-25	08-01-12	TEMPORARY CULVERT CROSSING, CONSTRUCTION EXIT, CONSTRUCTION FORD

EC-STR-30	INSTREAM DIVERSION (WITHOUT TRAFFIC)

EC-STR-30A	INSTREAM DIVERSION (WITH TRAFFIC)

EC-STR-31	05-04-22	TEMPORARY DIVERSION CHANNEL

EC-STR-31A	04-01-08	TEMPORARY DIVERSION CHANNEL DESIGN

EC-STR-32	08-01-12	TEMPORARY DIVERSION CULVERTS

EC-STR-33	08-01-12	SUSPENDED PIPE DIVERSION (DOWNSTREAM)

EC-STR-33A	08-01-12	SUSPENDED PIPE DIVERSION (UPSTREAM)

EC-STR-36	05-04-22	TURF REINFORCEMENT MAT FOR CHANNEL INSTALLATION

EC-STR-38	08-01-12	FLOATING TURBIDITY CURTAIN